{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["BPBP备用电源","BPSP太阳能电池板","BPWG风力发电装置","BPHT备用电源主机","BPCU备用电源控制箱"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BPBP备用电源","index":0,"n_rows":67,"n_cols":10,"rows_kept":67,"cut":false,"hidden":false,"merged":[[56,0,63,1],[32,1,50,1],[52,1,54,1],[32,0,54,0],[16,1,22,1],[55,0,55,1],[0,0,0,9],[1,0,1,1],[23,1,28,1],[29,1,31,1],[2,0,31,0],[2,1,15,1]]}
["备用电源"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数","总体","备用电源类型","BackupPowerType",null,"Enum","S","D1","1. UPS 2. EPS 99. 其他"]
[null,null,"使用方式","UseType",null,"Enum","M","D1","1. 后备式 2. 在线式 3. 在线互动式 99. 其他"]
[null,null,"是否有浪涌保护器","isSurgeProtector",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有维修旁路开关","isBypassSwitch",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"额定转换效率","RatedEff","%","Num","R","A2"]
[null,null,"抗震能力","SeismicCapacity",null,"Enum","S","D1","参考《10抗震设防烈度》"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"绝缘等级","InsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
[null,"输入","额定输入电压","RatedInU","V","Num","R","A2"]
[null,null,"额定输入电流","RatedInI","A","Num","M","A2"]
[null,null,"额定输入频率","RatedInFreq","Hz","Num","R","A2"]
[null,null,"输入相数","InPhaseNum","相","Num","R","A2"]
[null,null,"输入电压允许变动范围","AllowInURange","%","Numr","R","A6"]
[null,null,"输入频率允许变动范围","AllowInFreqRange","%","Numr","R","A6"]
[null,null,"输入功率因数","RatedInPFactor",null,"Num","R","A1"]
[null,"输出","额定输出电压","RatedOutU","V","Num","R","A2"]
[null,null,"额定输出电流","RatedOutI","A","Num","M","A2"]
[null,null,"额定输出频率","RatedOutFreq","Hz","Num","R","A2"]
[null,null,"输出相数","OutPhaseNum","相","Num","R","A2"]
[null,null,"输出功率因数","RatedOutPFactor",null,"Num","R","A1"]
[null,null,"输出整流器稳定精度","RectifierStableAccuracy","%","Num","R","A2"]
[null,"电池","是否有外置电池","isExternalBattery",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"电池后备时间","RatedBackupTime","h","Num","M","A2"]
[null,null,"电池转换时间","RatedTransTime","ms","Num","R","A2"]
["运行参数","瞬时参数","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"旁路开关状态","BypassSwitch",null,"Boolv","R","L","0. 关 1. 开"]
[null,null,"输入电压","InU","V","Inst","R","L"]
[null,null,"输入电流","InI","A","Inst","R","L"]
[null,null,"输入功率","InP","kW","Inst","R","L"]
[null,null,"输入频率","InFreq","Hz","Inst","R","L"]
[null,null,"输入功率因数","InPowerFactor",null,"Inst","R","L"]
[null,null,"输出电压","OutU","V","Inst","M","L"]
[null,null,"输出电流","OutI","A","Inst","M","L"]
[null,null,"输出功率","OutP","kW","Inst","M","L"]
[null,null,"输出频率","OutFreq","Hz","Inst","R","L"]
[null,null,"输出功率因数","OutPowerFactor",null,"Inst","R","L"]
[null,null,"蓄电池剩余电量","BatteryLeftE","Ah","Inst","S","L"]
[null,null,"蓄电池可持续时间","BatteryLastTime","h","Inst","S","L"]
[null,null,"电池温度","BatteryTemp","℃","Inst","M","L"]
[null,"关键指标","转换效率","Eff","%","Inst","R","M"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息",null,"系统报警","SysAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"输入故障报警","InErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"输出故障报警","OutErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"旁路故障报警","BypassErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"整流模块故障报警","RectifyModuleErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"电池故障报警","BatteryErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"逆变器故障报警","InverterErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[null,null,"监控故障报警","MonitorErrorAlarm",null,"Boolp","S","L","0. 正常 1. 报警"]
[]
[]
[null,null,null,"`"]

{"sheet":"BPSP太阳能电池板","index":1,"n_rows":53,"n_cols":10,"rows_kept":53,"cut":false,"hidden":false,"merged":[[51,0,51,1],[52,0,52,1],[0,0,0,9],[1,0,1,1],[37,0,50,0],[37,1,46,1],[47,1,50,1],[2,0,36,1]]}
["太阳能电池板"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"材料类型","MaterialType",null,"Enum","R","D1","1. 单晶硅电池板 2. 多晶硅电池板 3. 非晶硅电池板 4. 化学染料电池板 5. 柔性电池板 99. 其他"]
[null,null,"最大功率","MaxP","kW","Num","S","A2"]
[null,null,"最佳工作电压","RatedU","V","Num","M","A2"]
[null,null,"最佳工作电流","RatedI","A","Num","M","A2"]
[null,null,"最大系统电压","MaxSysU","V","Num","R","A2"]
[null,null,"开路电压","UOC","V","Num","R","A2"]
[null,null,"短路电流","ISC","A","Num","R","A2"]
[null,null,"电池数量","BatteryNum","个","Num","R","A2"]
[null,null,"功率温度系数","PTempCoeff","%/℃","Num","R","A2"]
[null,null,"工作电流温度系数","ITempCoeff","%/℃","Num","R","A2"]
[null,null,"工作电压温度系数","UTempCoeff","%/℃","Num","R","A2"]
[null,null,"开路电压温度系数","UOCTempCoeff","%/℃","Num","R","A2"]
[null,null,"短路电流温度系数","ISCTempCoeff","%/℃","Num","R","A2"]
[null,null,"有效辐射面积","RadiationArea","m2","Num","M","A2"]
[null,null,"吸收率","Absorptivity","%","Num","R","A2"]
[null,null,"发射率","Emissivity","%","Num","R","A2"]
[null,null,"额定转换效率","RatedEff","%","Num","M","A2"]
[null,null,"是否有蓄电池","isStorageBattery",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"蓄电池容量","StorageBatteryCap","Ah","Num","M","A2"]
[null,null,"是否有逆变器","isInverter",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"绝缘系数","InsulationCoeff","kΩ","Num","R","A2"]
[null,null,"放置朝向","Direct",null,"Enum","R","D1","见《6方向代码》"]
[null,null,"与水平方向倾角","HorizontalAngle","°","Num","R","A2"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"直流击穿电压","DCBreakdownU","V","Num","R","A2"]
[null,null,"交流击穿电压","ACBreakdownU","V","Num","R","A2"]
[null,null,"抗风力系数","WindResistanceCoeff","m/s","Num","R","A2"]
[null,null,"抗压能力","PressResistance","Pa","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"绝缘等级","InsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
["运行参数","瞬时参数","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"输出电压","OutU","V","Inst","M","L"]
[null,null,"输出电流","OutI","A","Inst","M","L"]
[null,null,"输出功率","OutP","kW","Inst","S","L"]
[null,null,"辐射强度","RadiationP","W/m2","Inst","R","L"]
[null,null,"转换效率","Eff","%","Inst","R","M"]
[null,"累计指标","累计发电量","AccOutE","kWh","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BPWG风力发电装置","index":2,"n_rows":48,"n_cols":10,"rows_kept":48,"cut":false,"hidden":false,"merged":[[46,0,46,1],[47,0,47,1],[0,0,0,9],[1,0,1,1],[32,0,45,0],[32,1,41,1],[42,1,45,1],[2,0,31,1]]}
["风力发电装置"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"风轮直径","WheelD","m","Num","R","A2"]
[null,null,"叶片材料","BladeMaterial",null,"Str","R","B1"]
[null,null,"叶片数目","BladeNum","个","Num","R","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"额定风速","RatedWindV","m/s","Num","S","A2"]
[null,null,"启动风速","StartWindV","m/s","Num","M","A2"]
[null,null,"运行风速范围","WorkWindVRange","m/s","Num","R","A2"]
[null,null,"极限风速","MaxWindV","m/s","Num","M","A2"]
[null,null,"额定转速","RatedRPM","rpm","Num","S","A2"]
[null,null,"工作电压","RatedWorkU","V","Num","R","A2"]
[null,null,"系统输出电压","RatedOutU","V","Num","S","A2"]
[null,null,"额定输出电流","RatedOutI","A","Num","M","A2"]
[null,null,"发电机类型","GeneratorType",null,"Str","R","B1"]
[null,null,"额定效率","RatedEff","%","Num","M","A2"]
[null,null,"限速方式","SpeedLimitMethod",null,"Str","R","B1"]
[null,null,"刹车系统","BrakeSys",null,"Str","R","B1"]
[null,null,"极限温度","LimitTemp","℃","Num","R","A2"]
[null,null,"设计寿命","ServiceLife","年","Num","R","A2"]
[null,null,"是否有蓄电池","isStorageBattery",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"蓄电池容量","StorageBatteryCap","Ah","Num","M","A2"]
[null,null,"是否有逆变器","isInverter",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"绝缘等级","InsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"噪声强度","Noise","dB(A)","Num","M","A2"]
[null,null,"振动烈度","Vibration","mm/s","Num","M","A2"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"输出电压","OutU","V","Inst","M","L"]
[null,null,"输出电流","OutI","A","Inst","M","L"]
[null,null,"输出功率","OutP","kW","Inst","S","L"]
[null,null,"风速","WindV","m/s","Inst","M","L"]
[null,null,"转换效率","Eff","%","Inst","R","M"]
[null,"累计指标","累计发电量","AccOutE","kWh","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BPHT备用电源主机","index":3,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[0,0,0,9],[1,0,1,1],[2,0,27,1],[28,0,39,0],[28,1,35,1],[36,1,39,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BPCU备用电源控制箱","index":4,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[0,0,0,9],[2,0,48,0],[60,0,60,1],[59,0,59,1],[1,0,1,1],[18,1,48,1],[49,0,58,0],[49,1,53,1],[54,1,58,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]