{"text_format":"2","workbook":"xlsx","n_sheets":6,"sheets":["MIHT多媒体主机","MIPL播放器","MIDS多媒体显示屏","MIST自助终端机","MIFE多媒体前端设备","MICU多媒体控制箱"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MIHT多媒体主机","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[1,0,1,1],[0,0,0,9],[28,0,39,0],[28,1,35,1],[36,1,39,1],[2,0,27,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MIPL播放器","index":1,"n_rows":32,"n_cols":10,"rows_kept":32,"cut":false,"hidden":false,"merged":[[30,0,30,1],[31,0,31,1],[0,0,0,9],[1,0,1,1],[16,0,29,0],[16,1,25,1],[26,1,29,1],[2,0,15,1]]}
["播放器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"多媒体接口","PlayerMultimediaPort",null,"Str","M","B1"]
[null,null,"是否有独立处理器","isPlayerSeparateProcessor",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否有数据存储功能","isPlayerDataStoreFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否具有无线通讯模块","isPlayerWirelessCommunication",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否具有GPS模块","isPlayerGPS",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"支持音频解码类型","PlayerAudioDecodeType",null,"MEnum","R","D2","1. MP2 2. MP3 3. AAC 4. 立体声 99. 其他 （可多选）"]
[null,null,"支持视频解码类型","PlayerVideoDecodeType",null,"MEnum","R","D2","1. mpg 2. avi 3. mp4 4. wmv 5. MPEG-1/2 6. MPEG4 7. H.264 99. 其他 （可多选）"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"当前播放类型","PlayType",null,"Enumv","M","L","1. 音频 2. 视频 99. 其他"]
[null,null,"当前解码类型","DecodeType",null,"Enumv","R","L","1. MP2 2. MP3 3. AAC 4. 立体声 5. mpg 6. avi 7. mp4 8. wmv 9. MPEG-1/2 10. MPEG4 11. H.264 99. 其他"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MIDS多媒体显示屏","index":2,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[43,0,43,1],[44,0,44,1],[33,0,42,0],[33,1,38,1],[39,1,42,1],[2,0,32,1]]}
["显示屏"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"平均功耗","RatedAveP","W","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","R","A2"]
[null,null,"控制系统","CtrlSys",null,"Str","R","B1"]
[null,null,"显示屏类型","DisplayType",null,"Enum","M","D1","1. LED 2. 液晶 99. 其他"]
[null,null,"显示颜色类型","ColorType",null,"Enum","M","D1","1. 单色 2. 双色 3. 彩色 99. 其他"]
[null,null,"显示屏尺寸","DisplaySize","英寸","Num","M","A2"]
[null,null,"有无触摸功能","isTouchFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"触摸类型","TouchType",null,"Enum","R","D1","1. 单点触摸 2. 多点触摸 99. 其他"]
[null,null,"是否具有红外触摸特性","isIRTouchFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"对比度","Contrast",null,"Num","R","A1"]
[null,null,"亮度","Luminance","cd/m2","Num","R","A2"]
[null,null,"亮度控制","LuminanceCtrl","级","Num","R","A2",null,"8位处理系统256级，矫正4096"]
[null,null,"水平/垂直视角","ViewAngle","°","Num","R","A2"]
[null,null,"支持最大分辨率","MaxResolution",null,"Num","M","A1"]
[null,null,"最佳视距","BestSightDistance","m","Num","R","A2"]
[null,null,"灰度等级","GrayScale",null,"Num","R","A1"]
[null,null,"显示颜色","ColorCap",null,"Num","R","A1"]
[null,null,"字体类型","FontType",null,"Str","R","B1"]
[null,null,"是否有英文显示","isEnglish",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有语音播报功能","isVoiceBroadcastFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"扫描频率","ScanFreq","MHz","Num","R","A2",null,"显示器每秒钟扫描的行数"]
[null,null,"图像传输速度","TransferSpeed","帧/s","Num","R","A2"]
[null,null,"屏幕刷新速率","RefreshRate","Hz","Num","R","A2",null,"显示器的刷新率指每秒钟出现新图像的数量"]
[null,null,"点间距","DotSpace","mm","Num","R","A2",null,"是指一种给定颜色的一个发光点与离它最近的相邻同色发光点之间的距离"]
[null,null,"像素密度","PixelDensity","个/m2","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MIST自助终端机","index":3,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[[49,0,49,1],[50,0,50,1],[0,0,0,9],[1,0,1,1],[39,0,48,0],[30,1,31,1],[27,1,29,1],[2,1,24,1],[39,1,44,1],[45,1,48,1],[2,0,38,0],[35,1,38,1]]}
["自助终端机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","显示屏","额定电压","RatedU","V","Num","R","A2"]
[null,null,"平均功耗","RatedAveP","W","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","R","A2"]
[null,null,"控制系统","CtrlSystem",null,"Str","R","B1"]
[null,null,"显示屏类型","DisplayType",null,"Enum","M","D1","1. LED 2. 液晶 99. 其他"]
[null,null,"显示屏尺寸","DisplaySize","英寸","Num","M","A2"]
[null,null,"有无触摸功能","isTouchFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"触摸类型","TouchType",null,"Enum","R","D1","1. 单点触摸 2. 多点触摸 99. 其他"]
[null,null,"是否具有红外触摸特性","isIRTouchFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"响应时间","ResponseTime","ms","Num","R","A2"]
[null,null,"对比度","Contrast",null,"Num","R","A1"]
[null,null,"亮度","Luminance","cd/m2","Num","R","A2"]
[null,null,"亮度控制","LuminanceCtrl","级","Num","R","A2",null,"8位处理系统256级，矫正4096"]
[null,null,"水平/垂直视角","ViewAngle","°","Num","R","A2"]
[null,null,"支持最大分辨率","MaxResolution",null,"Num","M","A1"]
[null,null,"最佳视距","BestSightDistance","m","Num","R","A2"]
[null,null,"灰度等级","GrayScale",null,"Num","R","A1"]
[null,null,"显示颜色","ColorCap",null,"Num","R","A1"]
[null,null,"扫描频率","ScanFreq","MHz","Num","R","A2",null,"显示器每秒钟扫描的行数"]
[null,null,"图像传输速度","TransferSpeed","帧/s","Num","R","A2"]
[null,null,"屏幕刷新速率","RefreshRate","Hz","Num","R","A2",null,"显示器的刷新率指每秒钟出现新图像的数量"]
[null,null,"点间距","DotSpace","mm","Num","R","A2",null,"是指一种给定颜色的一个发光点与离它最近的相邻同色发光点之间的距离"]
[null,null,"像素密度","PixelDensity","个/m2","Num","R","A2"]
[null,"IC读卡机","是否有IC读卡机","isICCardReader",null,"Bool","M","E1","0. 否 1. 是"]
[null,"密码键盘","是否有密码键盘","isPasswordKeyboard",null,"Bool","M","E1","0. 否 1. 是"]
[null,"身份证阅读器","是否有身份证阅读器","isIDCardRead",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"读卡时间","IDCardReadTime","s","Num","R","A2"]
[null,null,"最大读卡距离","IDCardMaxReadDistance","mm","Num","R","A2"]
[null,"打印机","是否有打印机","isPrinter",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"打印类型","PrinterType",null,"Enum","R","D1","1. 票据 2. 激光 99. 其他"]
[null,"指纹识别仪","是否有指纹识别仪","isTouchID",null,"Bool","M","E1","0. 否 1. 是"]
[null,"摄像头","是否有摄像头","isCamera",null,"Bool","M","E1","0. 否 1. 是"]
[null,"其他设备","其他设备","OtherEquip",null,"Str","R","B1"]
[null,"整机","防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MIFE多媒体前端设备","index":4,"n_rows":98,"n_cols":10,"rows_kept":98,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[2,0,83,0],[2,1,9,1],[10,1,16,1],[17,1,20,1],[21,1,29,1],[30,1,38,1],[39,1,44,1],[45,1,53,1],[96,0,96,1],[97,0,97,1],[54,1,65,1],[66,1,75,1],[76,1,83,1],[84,0,95,0],[84,1,91,1],[92,1,95,1]]}
["前端设备"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","前端设备类型","FrontEndEquipType",null,"Enum","S","D1","1. 高频头 2. 接收器 3. 混合器 4. 监视器 5. 功率放大器 6. 调制器 7. 分支分配器 8. 光端机 9. 播放器 99. 其他"]
[null,null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"高频头","是否包含高频头","isTuner",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"高频头输入频率","TunerInFreq","Hz","Num","R","A2",null,"高频头接收卫星发射信号的下行频率"]
[null,null,"高频头输出频率","TunerOutFreq","Hz","Num","R","A2",null,"输入信号的下行频率经高频头内部电路降频后，再由自身端口输出的中频频率"]
[null,null,"高频头本振频率","TunerLC","Hz","Num","R","A2",null,"高频头内部的本机振荡器产生的固定频率。"]
[null,null,"高频头噪声","TunerNoise","dB(A)","Num","R","A2",null,"放大器输入端和输出端信噪比的比值，表示信号经高频头后损失的信噪比，对接收系统整体性能起着重要的作用"]
[null,null,"高频头增益","TunerGain","dB(A)","Num","R","A2",null,"为弥补线路衰减及噪声影响，高频头必须具有较高的功率增益，一般要求大于60dB"]
[null,null,"高频头输出电压驻波比","TunerOutVSWR",null,"Num","R","A2",null,"表示匹配传输情况，驻波比过大会引起较强的反射，降低传输功率及稳定性，通常要求比值小于2.5"]
[null,"接收器","是否包含接收器","isReceiver",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"接收器输入频率","ReceiverInFreq","Hz","Num","R","A2",null,"高频头接收卫星发射信号的下行频率"]
[null,null,"接收器本振频率","ReceiverLC","Hz","Num","R","A2",null,"高频头内部的本机振荡器产生的固定频率。"]
[null,null,"接收器极化方式","ReceiverPolarType",null,"Enum","R","D1","1. 水平H 2. 垂直V 99. 其他"]
[null,"混合器","是否包含混合器","isMixer",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"混合器最低频率","MixerMinFreq","MHz","Num","R","A2"]
[null,null,"混合器最高频率","MixerMaxFreq","MHz","Num","R","A2"]
[null,null,"混合器频率响应","MixerFreqResponse","dB(A)","Num","R","A2"]
[null,null,"混合器隔离度","MixerIsolation","dB(A)","Num","R","A2"]
[null,null,"混合器输入反射损失","MixerInReflectLoss","dB(A)","Num","R","A2"]
[null,null,"混合器输出信号损失","MixerOutSignalLoss","dB(A)","Num","R","A2"]
[null,null,"混合器输入阻抗","MixerInImpedance","Ω","Num","R","A2"]
[null,null,"混合器输出阻抗","MixerOutImpedance","Ω","Num","R","A2"]
[null,"监视器","是否包含监视器","isMonitor",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"监视器像素","MonitorPixel",null,"Num","R","A1"]
[null,null,"监视器分辨率","MonitorResolution",null,"Num","R","A1"]
[null,null,"监视器扫描频率","MonitorScanFreq","Hz","Num","R","A2"]
[null,null,"监视器显像管尺寸","MonitorTubeSize","英寸","Num","R","A2"]
[null,null,"监视器清晰度","MonitorClarity",null,"Num","R","A1"]
[null,null,"监视器行频","MonitorLineFreq","Hz","Num","R","A2"]
[null,null,"监视器场频","MonitorFieldFreq","Hz","Num","R","A2"]
[null,null,"监视器白平衡度","MonitorRGB",null,"Num","R","A1"]
[null,"功放","是否包含功放","isAmplifier",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"功放额定输出功率","AmplifierRatedOutP","W","Num","R","A2",null,"指连续的正弦波功率，在1kHz正弦波输入及一定的负载下，\n谐波失真小于1%所输出的功率，表示成W/CH（瓦/声道）"]
[null,null,"功放总谐波失真","AmplifierTHD","%","Num","R","A2"]
[null,null,"功放转换速率","AmplifierInversion","V/μs","Num","R","A2",null,"单位时间上升的电压幅度"]
[null,null,"功放阻尼因子","AmplifierDampingFactor",null,"Num","R","A1",null,"功率放大器的负载阻抗（大功率管内部电阻加上音箱的接线线阻）"]
[null,null,"功放输出阻抗","AmplifierOutImpedance","Ω","Num","R","A2"]
[null,"调制器","是否包含调制器","isModulator",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"调制器图像载波输出电平","ModulatorCarrierOutLev","V","Num","R","A2"]
[null,null,"调制器最高频率","ModulatorMaxFreq","MHz","Num","R","A2"]
[null,null,"调制器最低频率","ModulatorMinFreq","MHz","Num","R","A2"]
[null,null,"调制器频率准确度","ModulatorFreqAccuracy","MHz","Num","R","A2"]
[null,null,"调制器射频输出反射损耗","ModulatorRFOutReflectLoss","dB(A)","Num","R","A2"]
[null,null,"调制器信噪比","ModulatorSNR","dB(A)","Num","R","A2"]
[null,null,"调制器带内平坦度","ModulatorBandFlatness","dB(A)","Num","R","A2"]
[null,null,"调制器调制度","ModulatorDegree","%","Num","R","A2"]
[null,"分支分配器","是否包含分支分配器","isDistributor",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"分配器带宽","DistributorBandWidth","MHz","Num","R","A2",null,"用来标识信号传输的数据传输能力、标识单位时间内通过链路的数据量、标识显示器的显示能力"]
[null,null,"分配器最小满增益","DistributorMinFullGain","dB(A)","Num","R","A2"]
[null,null,"分配器前置均衡器调节范围","DistributorPreEqualizerAdjustRange","dB(A)","Num","R","A6"]
[null,null,"分配器平坦度","DistributorFlatness","dB(A)","Num","R","A2",null,"在给定带宽范围内的增益“剧烈增加”和“快速下降”的数值"]
[null,null,"分配器噪声系数","DistributorNoiseFactor","dB(A)","Num","R","A2"]
[null,null,"分配器参考输出电平","DistributorRefOutLev","mV","Num","R","A2"]
[null,null,"分配器组合三次差拍比CTB","DistributorCTB","dB(A)","Num","R","A2",null,"电视信号通过放大器放大以后，其中任意三个频道的信号Axωx、Ayωy和Azωz相互作用可产生以下非线性失真产物k3AxAyAz(ωx±ωy±ωz)，以上式子中的\"ωx±ωy±ωz\"表示失真产物的频率是原来三个信号频率的和或者差，即三个频率的差拍"]
[null,null,"分配器交调比CM","DistributorCM","dB(A)","Num","R","A2"]
[null,null,"分配器组合二次差拍比CSO","DistributorCSO","dB(A)","Num","R","A2"]
[null,null,"分配器反射损耗","DistributorReflectLoss","dB(A)","Num","R","A2",null,"信号通过传输通道进入下一个器件的时候，通常不可能100%被下一个器件完全吸收，有一部分信号会反射出来向相反的方向传、回到原输出端，输入器件信号的电平与从器件反射出来的信号电平之差"]
[null,null,"分配器信号交流声比","DistributorSignalHumRatio","dB(A)","Num","R","A2"]
[null,"光端机","是否包含光端机","isOpticalEnd",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"光端机带宽","OpticalEndBandWidth","Hz","Num","R","A2"]
[null,null,"光端机误码率","OpticalEndBER","%","Num","R","A2"]
[null,null,"光端机信噪比","OpticalEndSNR","dB(A)","Num","R","A2"]
[null,null,"光端机信号阻抗","OpticalEndSignalImpedance","Ω","Num","R","A2"]
[null,null,"光端机信号电平","OpticalEndSignalLev","V","Num","R","A2"]
[null,null,"光端机光功率","OpticalEndLmP","dB(A)","Num","R","A2"]
[null,null,"光端机单模光纤允许最大链损","OpticalEndSMFMaxChainLoss","dB(A)","Num","R","A2"]
[null,null,"光端机信号接口","OpticalEndSignalPort",null,"Str","R","B1"]
[null,null,"光端机适用系统","OpticalEndSysType",null,"Enum","R","D1","1. 模拟系统 2. 数字系统 99. 其他"]
[null,"播放器","是否包含播放器","isPlayer",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"播放器多媒体接口","PlayerMultimediaPort",null,"Str","R","B1"]
[null,null,"播放器是否有独立处理器","isPlayerSeparateProcessor",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"播放器是否有数据存储功能","isPlayerDataStoreFunc",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"播放器是否有无线通讯模块","isPlayerWirelessCommunication",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"播放器是否有GPS模块","isPlayerGPS",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"播放器支持音频解码类型","PlayerAudioDecodeType",null,"MEnum","R","D2","1. MP2 2. MP3 3. AAC 4. 立体声 99. 其他 （可多选）"]
[null,null,"播放器支持视频解码类型","PlayerVideoDecodeType",null,"MEnum","R","D2","1. mpg 2. avi 3. mp4 4. wmv 5. MPEG-1/2 6. MPEG4 7. H.264 99. 其他 （可多选）"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MICU多媒体控制箱","index":5,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1],[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]