{"text_format":"2","workbook":"xlsx","n_sheets":9,"sheets":["GMHT车库主机","GMCU车库控制箱","GMCM车库摄像头","GMDS车库显示屏","GMGT进出闸机","GMMP机械车位","GMCP充电桩","GMPD车位检测器","GMGL车位引导灯"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GMHT车库主机","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[1,0,1,1],[0,0,0,9],[28,0,39,0],[28,1,35,1],[36,1,39,1],[2,0,27,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMCU车库控制箱","index":1,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1],[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMCM车库摄像头","index":2,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[[28,0,28,1],[29,0,29,1],[0,0,0,9],[1,0,1,1],[19,0,27,0],[19,1,24,1],[25,1,27,1],[2,0,18,1]]}
["摄像头"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统信号类型","SignalType",null,"Enum","S","D1","1. 模拟系统 2. 数字系统 99. 其他"]
[null,null,"分辨率","Resolution",null,"Num","S","A1"]
[null,null,"摄像头类型","CameraType",null,"Enum","S","D1","1. 枪机 2. 球机 3. 半球机 99. 其他"]
[null,null,"色彩","ColorType",null,"Enum","S","D1","1. 黑白 2. 彩色 99. 其他"]
[null,null,"灵敏度","Sensitivity",null,"Num","R","A1"]
[null,null,"清晰度","Clarity",null,"Num","R","A1"]
[null,null,"最低照度","MinLux","lux","Num","M","A2",null,"単位面积接受的光照强度"]
[null,null,"CCD尺寸","CCDSize","英寸","Num","R","A2",null,"摄像机靶面"]
[null,null,"光谱响应特性","SpectralResponseCharacter",null,"Str","R","B1"]
[null,null,"扫描制式","ScanMode ",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Boolv","M","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Inst","R","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","M","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMDS车库显示屏","index":3,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[[43,0,43,1],[44,0,44,1],[1,0,1,1],[33,1,38,1],[0,0,0,9],[33,0,42,0],[39,1,42,1],[2,0,32,1]]}
["显示屏"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"平均功耗","RatedAveP","W","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","R","A2"]
[null,null,"控制系统","CtrlSys",null,"Str","R","B1"]
[null,null,"显示屏类型","DisplayType",null,"Enum","M","D1","1. LED 2. 液晶 99. 其他"]
[null,null,"显示颜色类型","ColorType",null,"Enum","M","D1","1. 单色 2. 双色 3. 彩色 99. 其他"]
[null,null,"显示屏尺寸","DisplaySize","英寸","Num","M","A2"]
[null,null,"有无触摸功能","isTouchFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"触摸类型","TouchType",null,"Enum","R","D1","1. 单点触摸 2. 多点触摸 99. 其他"]
[null,null,"是否具有红外触摸特性","isIRTouchFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"对比度","Contrast",null,"Num","R","A1"]
[null,null,"亮度","Luminance","cd/m2","Num","R","A2"]
[null,null,"亮度控制","LuminanceCtrl","级","Num","R","A2",null,"8位处理系统256级，矫正4096"]
[null,null,"水平/垂直视角","ViewAngle","°","Num","R","A2"]
[null,null,"支持最大分辨率","MaxResolution",null,"Num","M","A1"]
[null,null,"最佳视距","BestSightDistance","m","Num","R","A2"]
[null,null,"灰度等级","GrayScale",null,"Num","R","A1"]
[null,null,"显示颜色","ColorCap",null,"Num","R","A1"]
[null,null,"字体类型","FontType",null,"Str","R","B1"]
[null,null,"是否有英文显示","isEnglish",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有语音播报功能","isVoiceBroadcastFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"扫描频率","ScanFreq","MHz","Num","R","A2",null,"显示器每秒钟扫描的行数"]
[null,null,"图像传输速度","TransferSpeed","帧/s","Num","R","A2"]
[null,null,"屏幕刷新速率","RefreshRate","Hz","Num","R","A2",null,"显示器的刷新率指每秒钟出现新图像的数量"]
[null,null,"点间距","DotSpace","mm","Num","R","A2",null,"是指一种给定颜色的一个发光点与离它最近的相邻同色发光点之间的距离"]
[null,null,"像素密度","PixelDensity","个/m2","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMGT进出闸机","index":4,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[[35,0,35,1],[36,0,36,1],[0,0,0,9],[1,0,1,1],[21,0,34,0],[30,1,34,1],[21,1,29,1],[2,0,20,1]]}
["进出闸机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"有无读卡机","isCardReader",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"有无出票机","isTicketMachine",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"有无摄像头","isCamera",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"进出方式","PassType",null,"Enum","S","D1","1. 刷卡 2. 拍照识别 3. 人工 99. 其他"]
[null,null,"读卡类型","CardType",null,"Enum","R","D1","1. ID卡 2. IC卡 3. CPU卡 99. 其他"]
[null,null,"管理门数","GateNum","个","Num","R","A2"]
[null,null,"最大临时放卡量","MaxTemporaryCardNum","个","Num","R","A2"]
[null,null,"读卡距离","CardReadDistance","mm","Num","R","A2"]
[null,null,"识别响应时间","IdentifyResponseTime","s","Num","R","A2"]
[null,null,"卡的寿命","CardLife ","年","Num","R","A2"]
[null,null,"数据传输率","DataTransferRate","MB/s","Num","R","A2"]
[null,null,"访问射频速率","AccessRFRate","MB/s","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"开闸状态","GateStatus",null,"Boolv","S","L","0. 关 1. 开"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计进出车次","AccCarTime","车次","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMMP机械车位","index":5,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[36,0,36,1],[37,0,37,1],[0,0,0,9],[1,0,1,1],[31,1,35,1],[22,1,30,1],[22,0,35,0],[2,0,21,1]]}
["机械车位"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"待机功率","RatedStandbyP","kW","Num","M","A2"]
[null,null,"运行功率","RatedRunP","kW","Num","S ","A2"]
[null,null,"停车位数","ParkingNum ","个","Num","S","A2"]
[null,null,"存取动作时间","AccessTime","min","Num","R","A2"]
[null,null,"适用车辆最大长度","CarMaxLength","mm","Num","M","A2"]
[null,null,"适用车辆最大宽度","CarMaxWidth","mm","Num","M","A2"]
[null,null,"适用车辆最大高度","CarMaxHeight","mm","Num","M","A2"]
[null,null,"传动方式","DriveType",null,"Enum","R","D1","1. 链条 2. 齿轮 99. 其他"]
[null,null,"横移运行速度","TranslationSpeed","m/s","Num","R","A2"]
[null,null,"转动运行速度","RotationSpeed","m/s","Num","R","A2"]
[null,null,"升降运行速度","LiftingSpeed","m/s","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"电机绝缘等级","MotorInsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"噪声强度","Noise","dB(A)","Num","M","A2"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","R","L"]
[null,null,"当前存放车数量","ParkingCarNum","辆","Inst","M","M"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计存车数量","AccParkingCarNum","辆","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime ","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMCP充电桩","index":6,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[[29,0,29,1],[30,0,30,1],[0,0,0,9],[1,0,1,1],[17,0,28,0],[17,1,24,1],[25,1,28,1],[2,0,16,1]]}
["充电桩"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定输出电压","RatedU","V","Num","S","A2"]
[null,null,"额定充电电流","RatedI","A","Num","S","A2"]
[null,null,"充电桩类型","EVType",null,"Enum","S","D1","1. 交流式 2. 直流式 3. 一体式 99. 其他"]
[null,null,"交流充电频率","AlternateChargingFreq","Hz","Num","R","A2"]
[null,null,"连接器动力线触头额定电压","ConnectorPowerLineRatedU","V","Num","R","A2"]
[null,null,"连接器动力线触头额定电流","ConnectorPowerLineRatedI","A","Num","R","A2"]
[null,null,"是否充电速度可选","isChargingRateOptional",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"快充电流","FastChargingI","A","Num","M","A2"]
[null,null,"慢充电流","SlowChargingI","A","Num","M","A2"]
[null,null,"连接器机械操作寿命","ConnectorMechanicalLife","次","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"绝缘等级","InsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"输出电压","U","V","Inst","M","L"]
[null,null,"输出电流","I","A","Inst","M","L"]
[null,null,"输出功率","P","kW","Inst","M","L"]
[null,"累计指标","累计输出电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"GMPD车位检测器","index":7,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[35,0,35,1],[33,0,34,1],[2,1,21,1],[0,0,0,9],[1,0,1,1],[2,0,26,0],[22,1,26,1],[27,0,32,0],[27,1,29,1],[30,1,32,1]]}
["车位检测器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","供电方式","PowerType",null,"Enum","S","D1","1. 电池供电 2. 交流电源供电 3. 直流电源供电 99. 其他"]
[null,null,"额定电压","RatedU","V","Num","M","A2"]
[null,null,"额定电流","RatedI","mA","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","M","A2"]
[null,null,"检测器类型","DetectorType",null,"Enum","S","D1","1. 环形线圈式 2. 波频式 3. 视频式 99. 其他"]
[null,null,"电池容量","BatteryCap","mAh","Num","R","A2",null,"针对电池供电"]
[null,null,"电池使用时间","BatteryUseTime","年","Num","M","A2",null,"针对电池供电"]
[null,null,"侦测距离","DetectDist","m","Num","M","A2"]
[null,null,"侦测角度","DetectAngle","⁰","Num","M","A2",null,"角度"]
[null,null,"有效通讯距离","CommunicateDist","m","Num","M","A2"]
[null,null,"距离最大误差","MaxDistErr","cm","Num","R","A2"]
[null,null,"车位满空判定时间","DetectTime","s","Num","R","A2"]
[null,null,"探测准确率","DetectAccuracy","%","Num","M","A2"]
[null,null,"通讯方式","CommunicateType",null,"Enum","M","D1","1. RS485 2. CAN 3. TTL 4. RS232 99. 其他"]
[null,null,"IO输出接口路数","LoopNum","路","Num","R","A2"]
[null,null,"通讯速率","CommunicateRate","bps","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"视频式","环境照度要求","MinIllum","Lux","Num","M","A2"]
[null,null,"图像压缩方式","ImageCompressType",null,"Enum","R","D1","1. JPEG 2. PNG 99. 其他"]
[null,null,"视频分辨率","VideoResolution","像素","Num","M","A2"]
[null,null,"视频帧率","VideoFrameRate","帧/s","Num","R","A2"]
[null,null,"视频码率","VideoBitrate","Mbps","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"车位是否占用","isOccupy",null,"Boolv","S","L","0. 未占用 1. 已占用"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数",null,"设备开关设定","EquipSwitchSet",null,"Boolp","M","L","0. 关闭 1. 开启"]
[null,null,"探测距离设定","DetectDistSet",null,"Nump","R","L"]
["报警消息"]

{"sheet":"GMGL车位引导灯","index":8,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[[23,1,26,1],[27,0,27,1],[28,0,28,1],[2,0,16,1],[0,0,0,9],[1,0,1,1],[17,0,26,0],[17,1,22,1]]}
["车位引导灯"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数",null,"电源频率","PowerFreq","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"安装位置","InstallType",null,"Enum","S","D1","1. 车位上方 2. 车位侧方 99. 其他"]
[null,null,"发光强度","LumIntensity","cd","Num","R","A2"]
[null,null,"灯光可视距离","VisualDist","m","Num","M","A2"]
[null,null,"车位空闲表示方式","FreeExpress",null,"Enum","S","D1","1. 熄灭 2. 闪烁 3. 常亮 99. 其他"]
[null,null,"车位空闲颜色","FreeColour",null,"Enum","S","D1","1. 红 2. 绿 3. 蓝 4. 黄 5. 紫 6. 青 7. 白 99. 其他"]
[null,null,"车位占用表示方式","OccupyExpress",null,"Enum","S","D1","1. 熄灭 2. 闪烁 3. 常亮 99. 其他"]
[null,null,"车位占用颜色","OccupyColour",null,"Enum","S","D1","1. 红 2. 绿 3. 蓝 4. 黄 5. 紫 6. 青 7. 白 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","R","L"]
[null,null,"车位状态","ParkingStatus",null,"Boolv","S","L","0. 空闲 1. 占用"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]