{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["LNHT服务器主机","LNRT路由器","LNEX交换机","LNHF硬件防火墙","LNAP无线AP点位"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LNHT服务器主机","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[41,0,41,1],[1,0,1,1],[0,0,0,9],[28,0,39,0],[28,1,35,1],[36,1,39,1],[40,0,40,1],[2,0,27,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"LNRT路由器","index":1,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[[39,0,39,1],[40,0,40,1],[30,0,38,0],[0,0,0,9],[1,0,1,1],[26,1,29,1],[30,1,35,1],[36,1,38,1],[2,0,29,0],[2,1,25,1]]}
["路由器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"是否有无线路由功能","isWirelessRouteFunc",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"接口类型","PortType",null,"Enum","M","D2","1. RS232 DTE/DCE接口 2. V.35 DTE/DCE接口 3. X.21 DTEDCE接口 4. RS449 DTE/DCE接口 5. EIA530 DTE接口 6. 10M以太网接口 7. 快速以太网接口 8. 10/100自适应以太网接口 9. 千兆以太网接口 10. ATM接口 11. POS接口 12. 令牌环接口 13. FDDI接口 14. E1/T1接口 15. E3/T3接口 16. ISDN接口 99. 其他 （可多选）"]
[null,null,"用户可用槽数","AvailableSlotNum","个","Num","R","A2",null,"模块化路由器中除CPU板、时钟板等必要系统板及系统板专用槽位外用户可以使用的插槽数"]
[null,null,"CPU主频","CPUFreq","MHz","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","R","A2"]
[null,null,"最大整机吞吐量","MaxTotThroughput","Mpps","Num","R","A2",null,"路由器整机的包转发能力"]
[null,null,"最大端口吞吐量","MaxPortThroughput","Mpps","Num","R","A2",null,"路由器的具体一个端口的包转发能力"]
[null,null,"支持网络协议","NetProtocolType",null,"MEnum","S","D2","1. TCP/IP协议 2. IPX/SPX协议 3. NetBEUI协议 99. 其他 （可多选）"]
[null,null,"背板结构","BackplaneStructureType",null,"Enum","R","D1","1. 共享背板结构 2. 交换式结构 99. 其他","背板是路由器输入端与输出端之间的物理通道"]
[null,null,"是否有线速转发能力（有无丢包）","isLinkSpeedForwardFunc",null,"Bool","R","E1","0. 无 1. 有","在达到端口最大速率的时候，路由器传输的数据没有丢包"]
[null,null,"丢包率","PacketLossRate","%","Num","R","A2",null,"丢包率是指在稳定的持续负荷情况下，由于包转发能力的限制而造成包丢失的概率"]
[null,null,"延时","Delay","s","Num","R","A2",null,"数据包的第一个比特进入路由器，到该帧的最后一个比特离开路由器所经历的时间，该时间间隔标志着路由器转发包的处理时间"]
[null,null,"最大带机数量","MaxLoadComputerNum","台","Num","R","A2",null,"路由器能负载的计算机数量"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"无线模块","发射频段","TransmitFreqBand",null,"Enum","R","D1","1. 2.4GHz 2. 5GHz 3. 双频 99. 其他"]
[null,null,"无线协议","WIFIProtocolType",null,"Enum","R","D1","1. IEEE802.11b 2. IEEE802.11g 3. IEEE802.11n 4. IEEE802.11a 5. IEEE802.11ac 99. 其他"]
[null,null,"天线数量","AntennaNum","根","Num","R","A2"]
[null,null,"天线增益","AntennaGain","dBi","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L"]
[null,null,"整机吞吐量","TotThroughput","Mpps","Inst","R","L"]
[null,null,"端口吞吐量","PortThroughput","Mpps","Inst","R","L"]
[null,null,"带机数量","LoadComputerNum","台","Inst","R","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"LNEX交换机","index":2,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[[47,0,47,1],[48,0,48,1],[0,0,0,9],[1,0,1,1],[27,0,46,0],[27,1,32,1],[42,1,46,1],[33,1,41,1],[2,0,26,1]]}
["交换机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"接口类型","PortType",null,"Enum","M","D2","1. RS232 DTE/DCE接口 2. V.35 DTE/DCE接口 3. X.21 DTEDCE接口 4. RS449 DTE/DCE接口 5. EIA530 DTE接口 6. 10M以太网接口 7. 快速以太网接口 8. 10/100自适应以太网接口 9. 千兆以太网接口 10. ATM接口 11. POS接口 12. 令牌环接口 13. FDDI接口 14. E1/T1接口 15. E3/T3接口 16. ISDN接口 99. 其他 （可多选）"]
[null,null,"CPU主频","CPUFreq","MHz","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","R","A2"]
[null,null,"背板带宽","BackplaneBandWidth","MB/s","Num","M","A2",null,"交换机接口处理器或接口卡和数据总线间所能吞吐的最大数据量"]
[null,null,"端口带宽","PortBandWidth","MB/s","Num","M","A2"]
[null,null,"端口数","PortNum","个","Num","M","A2"]
[null,null,"支持网络协议","NetProtocolType",null,"MEnum","S","D2","1. TCP/IP协议 2. IPX/SPX协议 3. NetBEUI协议 99. 其他 （可多选）"]
[null,null,"数据转发技术","DataForwardTechType",null,"Enum","R","D1","1. 直通转发技术 2. 存储转发技术 3. 碎片隔离式技术 99. 其他","交换机所采用的用于决定如何转发数据包的转发机制"]
[null,null,"是否有多个MAC硬件地址","isMultipleMACAddress",null,"Bool","R","E1","0. 否 1. 是","单MAC交换机主要设计用于连接最终用户，多MAC交换机在每个端口有足够存储体记忆多个硬件地址"]
[null,null,"最大MAC地址表大小","MaxMACAddressSize",null,"Num","R","A1"]
[null,null,"延时","Delay","s","Num","R","A2",null,"从交换机接收到数据包到开始向目的端口复制数据包之间的时间间隔"]
[null,null,"包转发率","PacketForwardRate","Mpps","Num","R","A2",null,"交换机转发数据包能力大小"]
[null,null,"是否可堆叠","isStack",null,"Bool","R","E1","0. 否 1. 是","堆叠指将一台以上的交换机组合起来共同工作，以便在有限的空间内提供尽可能多的端口"]
[null,null,"是否可模块化","isModule",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"整机吞吐量","TotThroughput","Mpps","Inst","R","L"]
[null,null,"端口吞吐量","PortThroughput","Mpps","Inst","R","L"]
[null,null,"带机数量","LoadComputerNum","台","Inst","R","L"]
[null,"CPU状态","节点5秒钟的CPU使用率","PortCPUUtilRatioIn5s","%","Inst","M","L"]
[null,null,"节点1分钟的CPU使用率","PortCPUUtilRatioIn1m","%","Inst","M","L"]
[null,null,"节点5分钟的CPU使用率","PortCPUUtilRatioIn5m","%","Inst","M","L"]
[null,null,"系统5秒内CPU使用率","SysCPUUtilRatioIn5s","%","Inst","M","L"]
[null,null,"系统1分钟内CPU使用率","SysCPUUtilRatioIn1m","%","Inst","M","L"]
[null,null,"系统5分钟内CPU使用率","SysCPUUtilRatioIn5m","%","Inst","M","L"]
[null,null,"系统5秒内CPU最高使用率","SysCPUMaxUtilRatioIn5s","%","Inst","R","L"]
[null,null,"系统1分钟内CPU最高使用率","SysCPUMaxUtilRatioIn1m","%","Inst","R","L"]
[null,null,"系统5分钟内CPU最高使用率","SysCPUMaxUtilRatioIn5m","%","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","M"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"LNHF硬件防火墙","index":3,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[36,0,36,1],[37,0,37,1],[0,0,0,9],[1,0,1,1],[26,0,35,0],[26,1,32,1],[33,1,35,1],[2,0,25,1]]}
["硬件防火墙"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"接口类型","PortType",null,"Enum","M","D2","1. RS232 DTE/DCE接口 2. V.35 DTE/DCE接口 3. X.21 DTEDCE接口 4. RS449 DTE/DCE接口 5. EIA530 DTE接口 6. 10M以太网接口 7. 快速以太网接口 8. 10/100自适应以太网接口 9. 千兆以太网接口 10. ATM接口 11. POS接口 12. 令牌环接口 13. FDDI接口 14. E1/T1接口 15. E3/T3接口 16. ISDN接口 99. 其他 （可多选）"]
[null,null,"接口数量","PortNum","个","Num","R","A2"]
[null,null,"CPU主频","CPUFreq","MHz","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","R","A2"]
[null,null,"网络吞吐量","NetThroughput","Mpps","Num","R","A2"]
[null,null,"并发连接数","ConcurrentConnectNum","个","Num","R","A2"]
[null,null,"每秒最大新建连接数","MaxNewConnectNumPerSecond","个","Num","R","A2"]
[null,null,"IPS吞吐量","IPSThroughput","Mpps","Num","R","A2"]
[null,null,"AV吞吐量","AVThroughput","Mpps","Num","R","A2"]
[null,null,"IPSec VPN吞吐量","IPSecVPNThroughput","Mpps","Num","R","A2"]
[null,null,"支持协议类型","ProtocolType",null,"Enum","M","D2","1. HTTP 2. FTP 3. SMTP 4. IMAP 5. POP3 6. TELNET 7. TCP 8. UDP 9. DNS 10. RPC 11. FINGER 12. MSSQL 13. ORACLE 14. NNTP 15. DHCP 16. LDAP 17. VoIP 18. NETBIOS 19. TFTP 20. SUNRPC 21. MSRPC 99. 其他 （可多选）"]
[null,null,"模块化功能","ModuleFunc",null,"MEnum","S","D2","1. 支持IPSEC VPN, SSL VPN功能 2. 入侵防御 3. 防病毒 4. QoS及应用识别控制功能 99. 其他 （可多选）"]
[null,null,"是否有身份认证设置","isAuthentication",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"报警状态","AlarmStatus",null,"Boolv","S","L","0. 正常 1. 报警"]
[null,null,"整机吞吐量","TotThroughput","Mpps","Inst","R","L"]
[null,null,"端口吞吐量","PortThroughput","Mpps","Inst","R","L"]
[null,null,"带机数量","LoadComputerNum","台","Inst","R","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"LNAP无线AP点位","index":4,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[[39,0,39,1],[40,0,40,1],[2,1,20,1],[0,0,0,9],[1,0,1,1],[2,0,28,0],[21,1,26,1],[27,1,28,1],[29,0,38,0],[29,1,34,1],[35,1,38,1]]}
["无线AP点位"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定电压","RatedU","V","Num","M","A2"]
[null,null,"额定电流","RatedI","mA","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","M","A2"]
[null,null,"供电方式","PowerSupplyMode",null,"Enum","S","E1","1. 本地供电 2. PoE供电 99. 其他"]
[null,null,"安装方式","InstallationMode",null,"Enum","M","D1","1. 吸顶式 2. 面板式 3. 挂壁式 99. 其他"]
[null,null,"适用面积","ApplicableArea","m2","Num","S","A2"]
[null,null,"无线传输速率","WirelessTransmissionRate","Mbps","Num","M","A2"]
[null,null,"整机最大接入用户数","MaxUsers","个","Num","S","A2"]
[null,null,"推荐最佳接入用户数","BestUsers","个","Num","S","A2",null,"用户体验最佳"]
[null,null,"支持网络协议","NetProtocolType",null,"MEnum","M","D2","1. TCP/IP协议 2. IPX/SPX协议 3. NetBEUI协议 99. 其他 （可多选）"]
[null,null,"是否可作网桥","As A Bridge?",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"工作模式","WorkingMode",null,"MEnum","R","D2","1. 点对点无线桥接模式 2. 点对多点无线桥接模式 3. 中继模式 4. 无线分布系统 5. 可调整的输出功率控制 99. 其他 （可多选）"]
[null,null,"输入输出驻波比","SWR",null,"Num","R","A1"]
[null,null,"开启/关闭时间","Open/CloseTtime","μs","Num","R","A2"]
[null,null,"指示灯颜色","LightColor",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"发射指标","频率范围","FrequencyRange","MHz","Numr","M","A6"]
[null,null,"输出功率","OutputP","dBm","Num","R","A2"]
[null,null,"最大输入电平","MaxInputLevel","dBm","Num","R","A2"]
[null,null,"线性增益","LinearGain","dB","Num","R","A2"]
[null,null,"增益平坦度","GainFlatness","dB","Num","R","A2"]
[null,null,"EVM","EVM","%","Num","R","A2",null,"误差向量幅度"]
[null,"接收指标","接收增益","ReceivingGain","dB","Num","R","A2"]
[null,null,"典型噪声系数","NoiseFactor","dB","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","mA","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"数据上传速度","DownloadSpeed","Mbps","Inst","S","L"]
[null,null,"数据下载速度","UploadSpeed","Mbps","Inst","S","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]