{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["FGPA燃气调压箱","FGLP液化石油气瓶"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FGPA燃气调压箱","index":0,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[[29,0,29,1],[30,0,30,1],[16,0,28,0],[0,0,0,9],[1,0,1,1],[16,1,24,1],[25,1,28,1],[2,0,15,1]]}
["燃气调压箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"结构类型","StructureType",null,"Enum","M","D1","1. 单路调压箱无旁通 2. 单路调压箱有旁通 3. 双路调压箱无旁通 4. 双路调压箱有旁通 5. 多路调压箱 99. 其他"]
[null,null,"适用介质","GasType",null,"Enum","S","D1","1. 天然气 2. 城市煤气 3. 液化石油气 4. LPG混空气 99. 其他"]
[null,null,"额定流量","RatedFlow","m3/h","Num","S","A2"]
[null,null,"进口压力上限","InPressUpLimit","MPa","Num","M","A2"]
[null,null,"进口压力下限","InPressLowLimit","MPa","Num","M","A2"]
[null,null,"出口压力上限","OutPressUpLimit","MPa","Num","M","A2"]
[null,null,"出口压力下限","OutPressLowLimit","MPa","Num","M","A2"]
[null,null,"关闭压力","OffPress","MPa","Num","S","A2"]
[null,null,"调压精度","AdjustPrecision","%","Num","M","A2"]
[null,null,"过滤精度","FiltPrecision","μm","Num","R","A2"]
[null,null,"进口管径","InPipeDiameter","mm","Num","R","A2"]
[null,null,"出口管径","OutPipeDiameter","mm","Num","R","A2"]
[null,null,"适应下游用户数","RatedUserNum","户","Num","R","A2"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"燃气流量","GasFlow","m3/h","Inst","M","L"]
[null,null,"燃气温度","GasTemp","℃","Inst","R","L"]
[null,null,"进口压力","InPress","MPa","Inst","M","L"]
[null,null,"出口压力","OutPress","MPa","Inst","M","L"]
[null,"累计指标","累计供气量","AccSupplyGasVolume","m3","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FGLP液化石油气瓶","index":1,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[[20,0,20,1],[21,0,21,1],[0,0,0,9],[1,0,1,1],[2,0,8,1],[15,1,19,1],[9,0,19,0],[9,1,14,1]]}
["液化石油气瓶"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"钢瓶内直径","CylinderInDiameter","mm","Num","R","A2"]
[null,null,"底座外直径","BaseOutDiameter","mm","Num","R","A2"]
[null,null,"护罩外直径","ShieldOutDiameter","mm","Num","R","A2"]
[null,null,"公称容积","NominalCap","L","Num","S","A2"]
[null,null,"公称工作压力","NominalWorkPress","MPa","Num","M","A2"]
[null,null,"最大出气流量","MaxGasOutFlow","m3/h","Num","M","A2"]
[null,null,"充装重量","ChargeWeight","kg","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"阀门开度","ValveOpening","%","Inst","R","L"]
[null,null,"出气流量","GasOutFlow","m3/h","Inst","R","L"]
[null,null,"当前储气压力","GasStorePress","MPa","Inst","R","L"]
[null,null,"当前储气量","GasStoreVolume","kg","Inst","R","L"]
[null,"累计指标","累计用气量","AccGasConsum","kg","Acc","R","M"]
[null,null,"累计剩余气量","AccGasRemain","kg","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","R","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]