{"text_format":"2","workbook":"xlsx","n_sheets":13,"sheets":["SECB组合式传感器","SETP温度传感器","SERH湿度传感器","SEPS压力传感器","SECT浓度传感器","SESP速度传感器","SEDP位移传感器","SEFL流量传感器","SEHT热量传感器","SEEE电度传感器","SESD声音传感器","SEVD图像传感器","SEPF人流量传感器"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SECB组合式传感器","index":0,"n_rows":318,"n_cols":10,"rows_kept":318,"cut":false,"hidden":false,"merged":[[102,0,115,0],[116,0,131,0],[113,1,115,1],[102,1,112,1],[116,1,126,1],[127,1,131,1],[0,0,0,9],[49,0,91,0],[53,1,56,1],[73,1,75,1],[76,1,79,1],[49,1,52,1],[57,1,59,1],[60,1,62,1],[1,0,1,1],[2,0,46,1],[92,0,101,0],[47,0,48,1],[89,1,91,1],[92,1,98,1],[99,1,101,1],[63,1,72,1],[80,1,88,1],[171,0,193,0],[171,1,183,1],[184,1,193,1],[132,0,140,0],[154,0,170,0],[132,1,137,1],[154,1,162,1],[163,1,170,1],[141,0,153,0],[141,1,150,1],[151,1,153,1],[138,1,140,1],[307,0,317,0],[307,1,312,1],[313,1,317,1],[305,1,306,1],[194,1,206,1],[278,1,280,1],[281,1,304,1],[265,0,280,0],[265,1,266,1],[267,1,273,1],[274,1,277,1],[194,0,264,0],[207,1,264,1],[281,0,306,0]]}
["组合式传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"测试物理量","PhysicalQuantityType",null,"MEnum","S","D2","1. 温度 2. 湿度 3. 压力 4. 浓度 5. 速度 6. 位移 7. 流量 8. 热量 9. 电度 10. 声音 11. 图像 12. 人流量 99. 其他 （多选）"]
[null,null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["温度传感器","技术参数-温度通用","温度传感器种类","TempSensorType",null,"Enum","R","D1","1. 热电偶温度传感器 2. 热敏电阻温度传感器 3. 电阻温度传感器 4. IC温度传感器 5. 玻璃管温度计 6. 压力式温度计 7. 红外光电测温仪 8. 热色液晶测温仪 9. 全息干涉技术测温 99. 其他"]
[null,null,"温度测量上限","TempUpperLimit","℃","Num","M","A2"]
[null,null,"温度测量下限","TempLowerLimit","℃","Num","M","A2"]
[null,null,"温度传感器传递函数","TempTransFunc",null,"Str","R","B1"]
[null,"技术参数-热电偶温度传感器","热电偶温度传感器分度号","TempThermocoupleGraduation",null,"Enum","R","D1","1. S 2. R 3. B 4. N 5. K 6. E 7. J 8. T 99. 其他","不同的分度号表示不同的材料"]
[null,null,"热电偶温度传感器布置方式","TempThermocoupleInstallType",null,"Enum","R","D1","1. 触壁式 2. 非触壁式 3. 暴露式 99. 其他"]
[null,null,"热电偶温度传感器结构形式","TempThermocoupleStructureType",null,"Enum","R","D1","1. 普通热电偶 2. 耐磨热电偶 3. 铠装热电偶 4. 防爆热电偶 99. 其他"]
[null,null,"热电偶温度传感器插入深度","TempThermocoupleInsertDepth","mm","Num","R","A2"]
[null,"技术参数-热敏电阻温度传感器","热敏电阻温度传感器材料类型","TempThermistorMaterial",null,"Enum","R","D1","1. PTC 2. RTC 99. 其他"]
[null,null,"热敏电阻温度传感器电阻标称值","TempThermistorResistance","Ω","Num","R","A2"]
[null,null,"热敏电阻温度传感器耗散系数","TempThermistorDissipationCoeff","mW/℃","Num","R","A2"]
[null,"技术参数-电阻温度传感器","电阻温度传感器材料","TempResistorMaterial",null,"Enum","R","D1","1. 铂 2. 铜 3. 镍4. 铁镍合金 99. 其他"]
[null,null,"电阻温度传感器标称值","TempResistorResistance","Ω","Num","R","A2",null,"0℃时的电阻"]
[null,null,"电阻温度传感器耗散系数","TempResistorDissipationCoeff","mW/℃","Num","R","A2"]
[null,"技术参数-IC温度传感器","IC温度传感器种类","TempICSensorType",null,"Bool","R","E1","0. 模拟IC温度传感器 1. 数字IC温度传感器"]
[null,null,"IC温度传感器AD转换位数","TempICADConverseBit","bit","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器标称频率","TempICFreq","Hz","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出PWM低电压","TempICOutPWMLowU","V","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出PWM高电压","TempICOutPWMHighU","V","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器上升时间","TempICRiseTime","μs","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器下降时间","TempICFallTime","μs","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器电源抑制比","TempICPSRR","dB(A)","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出增益","TempICOutGain","dB(A)","Num","R","A2",null,"模拟"]
[null,null,"IC温度传感器0℃输出偏移","TempICOutOffset","mV","Num","R","A2",null,"模拟"]
[null,"技术参数-玻璃管式温度计","玻璃管温度传感器内部液体种类","TempTubeLiquidType",null,"Enum","R","D1","1. 水银 2. 有机液体 99. 其他"]
[null,null,"玻璃管温度传感器内部长度","TempTubeLength","mm","Num","R","A2"]
[null,null,"玻璃管温度传感器内部直径","TempTubeDiameter","mm","Num","R","A2"]
[null,"技术参数-压力式温度计","压力式温度传感器尾部长度","TempPressTailLength","mm","Num","R","A2"]
[null,null,"压力式温度传感器温包材料","TempPressBulbMaterial",null,"Enum","R","D1","1. 铜 2. 不锈钢 99. 其他"]
[null,null,"压力式温度传感器毛细管材料","TempPressCapillaryMaterial",null,"Enum","R","D1","1. 铜 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"压力式温度传感器温包插入深度范围","TempPressInsertDepthRange","mm","Num","R","A6"]
[null,"技术参数-红外测温仪","红外温度传感器探测器类型","TempInfraredDetectorType",null,"Bool","R","E1","0. 非制冷红外焦平面 1. 制冷红外焦平面"]
[null,null,"红外温度传感器探测元数量","TempInfraredDetectorNum",null,"Num","R","A3",null,"eg：160*220分别代表长宽方向的探测元数量"]
[null,null,"红外温度传感器响应波段","TempInfraredResponseBand","μm","Num","R","A2"]
[null,null,"红外温度传感器焦距","TempInfraredFocalDistance","mm","Num","R","A2"]
[null,null,"红外温度传感器NETD","TempInfraredNETD","mK","Num","R","A2"]
[null,null,"红外温度传感器IFOV","TempInfraredIFOV","mrad","Num","R","A2"]
[null,null,"红外温度传感器视场角","TempInfraredFieldAngle","°","Num","R","A4",null,"eg：3.6˚*1.2˚"]
[null,null,"红外温度传感器是否有自动调焦功能","isTempInfraredAutoFocusFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"红外温度传感器显示图像模式","TempInfraredDisplayType",null,"Enum","R","D1","1. 红外 2. 可见光 3. MIF 4. PIP 99. 其他"]
[null,"运行参数","温度传感器输出电压","TempOutU","V","Inst","R","L"]
[null,null,"温度传感器输出电流","TempOutI","A","Inst","R","L"]
[null,null,"温度传感器温度测量值","Temp","℃","Inst","S","L"]
["湿度传感器","技术参数","湿度传感器种类","RHSensorType",null,"Enum","R","D1","1. 电解质湿度传感器 2. MOS陶瓷湿度传感器 3. 高分子湿度传感器 4. 热敏电阻式湿度传感器 5. 红外吸收式湿度传感器 6. 微波式湿度传感器 7. 超声波湿度传感器 99. 其他"]
[null,null,"湿度测量上限","RHUpperLimit","%RH","Num","M","A2"]
[null,null,"湿度测量下限","RHLowerLimit","%RH","Num","M","A2"]
[null,null,"湿度传感器传递函数","RHTransFunc",null,"Str","R","B1"]
[null,null,"湿度传感器湿滞回差","RHHysteresisReturnDifference",null,"Num","R","A1"]
[null,null,"湿度传感器温度系数","RHTempCoeff","%RH/℃","Num","R","A2"]
[null,null,"湿度传感器外壳材料","RHShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,"运行参数","湿度传感器输出电压","RHOutU","V","Inst","R","L"]
[null,null,"湿度传感器输出电流","RHOutI","A","Inst","R","L"]
[null,null,"湿度传感器相对湿度测量值","RH","%RH","Inst","S","L"]
["压力传感器","技术参数","压力传感器种类","PressSensorType",null,"Enum","R","D1","1. 液柱式压力计 1.1 U形管压力计 1.2 斜管微压计 1.3 单管压力计 2. 弹性压力计 2.1 膜片压力计 2.1.1 电容式压力传感器 2.1.2 光纤式压力传感器 2.1.3 力矩平衡式压力变送器 2.2 弹簧管 2.2.1 弹簧管压力表 2.2.2 霍尔远传压力表 2.3 波纹管 3. 电气式压力计 3.1 压电式压力传感器 3.2 应变式压力传感器 3.3 压阻式压力传感器 4. 负荷式压力计 4.1 活塞式压力计 4.2 钟罩式微压计 99. 其他"]
[null,null,"压力传感器介质","PressMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 2. 液体\n2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）"]
[null,null,"压力测量上限","PressUpperLimit","Pa","Num","M","A2"]
[null,null,"压力测量下限","PressLowerLimit","Pa","Num","M","A2"]
[null,null,"压力传感器传递函数","PressTransFunc",null,"Str","R","B1"]
[null,null,"压力传感器温度补偿","PressTempCompensation","℃","Num","R","A2"]
[null,null,"压力传感器负载电阻","PressLoadResistance","Ω","Num","R","A2"]
[null,null,"压力传感器绝缘电阻","PressInsulationResistance","Ω","Num","R","A2"]
[null,null,"压力传感器输出负载","PressOutLoad","Ω","Num","R","A2"]
[null,null,"压力传感器温漂系数","PressTempDriftCoeff","mm","Num","R","A2"]
[null,null,"压力传感器外壳材料","PressShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,"运行参数","压力传感器输出电压","PressOutU","V","Inst","R","L"]
[null,null,"压力传感器输出电流","PressOutI","A","Inst","R","L"]
[null,null,"压力传感器压力测量值","Press","Pa","Inst","S","L"]
["浓度传感器","技术参数","浓度传感器测量对象","ConcentrateSensorType",null,"MEnum","S","D2","1. 一氧化碳 2. 二氧化碳 3. 二氧化硫 4. 氮氧化物 5. 甲醛 6. 苯 7. 总挥发性有机化合物 8. 总悬浮颗粒 9. 可吸入颗粒物 10. 烟雾浓度 11. 生物微粒 12. 水硬度 13. PH值 14. SS值 15. COD值 99. 其他 （可多选）","硬度：水总硬度是指水中Ca2+、Mg2+的总量；SS值：水中悬浮物；COD值：化学需氧量，是在一定的条件下，采用一定的强氧化剂处理水样时，所消耗的氧气的量，表示水中还原性物质多少"]
[null,null,"浓度传感器介质种类","ConcentrateMediumType",null,"Enum","M","D1","1. 气体 2. 液体 99. 其他"]
[null,null,"浓度传感器是否有报警功能","isAlarmFunc",null,"Bool","S","E1","0. 否  1. 是"]
[null,null,"浓度传感器最大报警电流","MaxAlarmI","A","Num","R","A2"]
[null,null,"浓度测量上限","ConcentrateUpperLimit",null,"Num","M","A1"]
[null,null,"浓度测量下限","ConcentrateLowerLimit",null,"Num","M","A1"]
[null,null,"浓度测量单位类型","ConcentrateMeasureUnitType",null,"MEnum","S","D2","1. ppm 2. μg/m3 3. μg/L 4. mmol/L 99. 其他 （多选）","液、气体中的气体ppm；气体中的颗粒物μg/m3；液体中的悬浮物ug/L；液体中离子mmol/L"]
[null,null,"浓度传感器传递函数","ConcentrateTransFunc",null,"Str","R","B1"]
[null,null,"浓度传感器外壳材料","ConcentrateShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"浓度传感器采样流量","ConcentrateSampleFlow","mL/min","Num","R","A2"]
[null,null,"浓度传感器采样方式","ConcentrateSampleMode",null,"Str","R","B1"]
[null,"运行参数","浓度传感器是否正在报警","isConcentrateAlarm",null,"Boolv","S","L","0. 否  1. 是"]
[null,null,"浓度传感器输出电压","ConcentrateOutU","V","Inst","R","L"]
[null,null,"浓度传感器输出电流","ConcentrateOutI","A","Inst","R","L"]
[null,null,"浓度传感器浓度测量单位","ConcentrateUnit",null,"Enumv","S","D1","1. ppm 2. μg/m3 3. μg/L 4. mmol/L 99. 其他"]
[null,null,"浓度传感器浓度测量值","Concentrate",null,"Inst","S","L"]
["速度传感器","技术参数","速度传感器原理类型","VSensorType",null,"Enum","R","D1","1. 机械式风速仪 2. 热线风速仪 3. 测压管 4. 激光多普勒测速仪 99. 其他"]
[null,null,"速度传感器介质种类","VMediumType",null,"Enum","S","D1","1. 气体 2. 液体 99. 其他"]
[null,null,"速度传感器外壳材料","VShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"速度测量上限","VUpperLimit","m/s","Num","M","A2"]
[null,null,"速度测量下限","VLowerLimit","m/s","Num","M","A2"]
[null,null,"速度传感器传递函数","VTransFunc",null,"Str","R","B1"]
[null,"运行参数","速度传感器输出电压","VOutU","V","Inst","R","L"]
[null,null,"速度传感器输出电流","VOutI","A","Inst","R","L"]
[null,null,"速度传感器速度测量值","V","m/s","Inst","S","L"]
["位移传感器","技术参数","位移传感器原理类型","DisplaceSensorType",null,"Enum","R","D1","1. 金属膜 2. 导电塑料 3. 光电式 4. 磁敏式 5. 金属玻璃轴 6. 绕线式 7. 数字激光式 99. 其他","应用领域：自动门（列车及大厅）；拉绳/拉线；电梯平层；升降机；开关窗记录仪"]
[null,null,"位移传感器传递函数","DisplaceTransFunc",null,"Str","R","B1"]
[null,null,"位移测量上限","DisplaceUpperLimit","mm","Num","M","A2"]
[null,null,"位移测量下限","DisplaceLowerLimit","mm","Num","M","A2"]
[null,null,"位移传感器标称电阻","DisplaceResistance","kΩ","Num","R","A2"]
[null,null,"位移传感器阻值公差","DisplaceResistanceTolerance","%","Num","R","A2"]
[null,null,"位移传感器绝缘电阻","DisplaceInsulationResistance","MΩ","Num","R","A2"]
[null,null,"位移传感器绝缘强度","DisplaceInsulationStrength","kV/mm","Num","R","A2"]
[null,null,"位移传感器振动","DisplaceVibration","Hz","Num","R","A2"]
[null,null,"位移传感器驱动力（水平方向）","DisplaceDriveForce ","N","Num","R","A2"]
[null,"运行参数","位移传感器输出电压","DisplaceOutU","V","Inst","R","L"]
[null,null,"位移传感器输出电流","DisplaceOutI","A","Inst","R","L"]
[null,null,"位移传感器位移测量值","Displace","m ","Inst","S","L"]
["流量传感器","技术参数","流量传感器原理类型","FlowSensorType",null,"Enum","R","D1","1. 压差式 1.1 孔板流量计 1.2 喷嘴 1.3 文丘利管 1.4 V形内锥式流量计 1.5 转子流量计 1.6 动压平均管 2. 叶轮式 2.1 水表 2.2 涡轮流量计 3. 电磁流量计 4. 超声波流量计 5. 涡街流量计 6. 容积流量计 6.1 腰轮流量计 6.2 转式气体流量计 6.3 薄膜式气体流量计 99. 其他"]
[null,null,"流量传感器介质种类","FlowMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 1.5 蒸汽 2. 液体 2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）"]
[null,null,"流量测量上限","FlowUpperLimit",null,"Num","M","A2"]
[null,null,"流量测量下限","FlowLowerLimit",null,"Num","M","A2"]
[null,null,"流量测量单位类型","FlowMeasureUnitType",null,"MEnum","S","D2","1. kg/h 2. m3/s 3. kgf/h 99. 其他 （多选）"]
[null,null,"流量传感器传递函数","FlowTransFunc",null,"Str","R","B1"]
[null,null,"流量传感器内部电容","FlowInElecCap","pF","Num","R","A2"]
[null,null,"流量传感器温度变化响应时间","FlowTempResponseTime","s","Num","R","A2"]
[null,null,"流量传感器温度梯度","FlowTempGradient","℃/min","Num","R","A2"]
[null,"运行参数","流量传感器输出电压","FlowOutU","V","Inst","R","L"]
[null,null,"流量传感器输出电流","FlowOutI","A","Inst","R","L"]
[null,null,"流量传感器流速测量值","FlowSpeed","m/s","Inst","M","L"]
[null,null,"流量传感器流量测量值","Flow","m3/h","Inst","S","L"]
[null,null,"流量传感器累计流量测量值","FlowAccVolume","m3","Acc","M","L",null,"正向计费"]
[null,null,"流量传感器累计金额测量值","FlowAccCost","元","Acc","M","L",null,"正向计费"]
[null,null,"流量传感器剩余流量测量值","FlowSurplusVolume","m3","Acc","M","L",null,"扣除计费"]
[null,null,"流量传感器剩余金额测量值","FlowSurplusCost","元","Acc","M","L",null,"扣除计费"]
["热量传感器","技术参数","热量传感器功能类型","HeatFuncType",null,"Enum","M","D1","1. 流体单热量表 2. 流体冷热量表 3. 热流密度计 99. 其他"]
[null,null,"热量传感器原理类型","HeatPrincipleType",null,"Enum","R","D1","1. 机械式热量表 2. 超声波式热量表 3. 电磁式热量表 99. 其他","流体量表"]
[null,null,"热量传感器结构类型","HeatStructType",null,"Enum","R","D1","1. 整体式热量表 2. 组合式热量表 3. 紧凑式热量表 99. 其他","流体量表"]
[null,null,"热量传感器功率类型","HeatPowerType",null,"Enum","R","D1","1. 户用量表（DN≤40mm） 2. 工业用量表（DN>40mm） 99. 其他","流体量表"]
[null,null,"热量传感器精度等级","HeatPrecisionType",null,"Enum","R","D1","1. 一级表 2. 二级表 3. 三级表 99. 其他","流体量表"]
[null,null,"热量传感器介质种类","HeatMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 2. 液体\n2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）","流体量表"]
[null,null,"热量传感器热传递类型","HeatTransType",null,"MEnum","R","D2","1. 热传导 2. 热辐射 3. 热对流 99. 其他 （可多选）","热流计"]
[null,null,"热量传感器数量类型","HeatSensorNumType",null,"Bool","R","E1","0. 单通道热流计 1. 多通道热流计","热流计"]
[null,null,"热量传感器外形类型","HeatShapeType",null,"Enum","R","D1","1. 手持式热流计 2. 便携式热流计 99. 其他","热流计"]
[null,null,"热（流）量测量上限","HeatUpperLimit","kW/m2","Num","M","A2"]
[null,null,"热（流）量测量下限","HeatLowerLimit","kW/m2","Num","M","A2"]
[null,null,"热量传感器传递函数","HeatTransFunc",null,"Str","R","B1"]
[null,null,"热量传感器响应时间","HeatResponseTime","s","Num","R","A2"]
[null,"运行参数","热量传感器输出电压","HeatOutU","V","Inst","R","L"]
[null,null,"热量传感器输出电流","HeatOutI","A","Inst","R","L"]
[null,null,"热量传感器温差测量值","HeatTempDifference","℃","Inst","M","L",null,"流体量表"]
[null,null,"热量传感器流量测量值","HeatFlow","m3/h","Inst","M","L",null,"流体量表"]
[null,null,"热量传感器热量测量值","Heat","kW","Inst","S","L"]
[null,null,"热量传感器热流量测量值","HeatIndensity","kW/m2","Inst","S","L"]
[null,null,"热量传感器累计热量测量值","HeatAccHeat","kWh","Acc","M","L",null,"正向计费"]
[null,null,"热量传感器累计金额测量值","HeatAccCost","元","Acc","M","L",null,"正向计费"]
[null,null,"热量传感器剩余热量测量值","HeatSurplusHeat","kWh","Acc","M","L",null,"扣除计费"]
[null,null,"热量传感器剩余金额测量值","HeatSurplusCost","元","Acc","M","L",null,"扣除计费"]
["电度传感器","技术参数","电表种类","ElecMeterType",null,"Enum","S","D1","1. 单向电能表 2. 三相三线电能表 3. 三相四线电能表 4. 综保电表 5. 计费电表 99. 其他"]
[null,null,"电表准确度等级","ElecAccuracyLev",null,"Enum","R","D1","1. 1级 2. 2级 99. 其他"]
[null,null,"电表是否有多费率功能","isElecMultiRateFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"电表是否有预付费功能","isElecPrepayFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"电表PT变比","ElecPTRatio",null,"Num","M","A1"]
[null,null,"电表CT变比","ElecCTRatio",null,"Num","M","A1"]
[null,null,"电表标准参比电压","ElecRatedRefU","V","Num","R","A2"]
[null,null,"电表标准参比频率","ElecRatedRefFreq","Hz","Num","R","A2"]
[null,null,"电表最大电流","ElecMaxI","A","Num","R","A2"]
[null,null,"电表潜动电压","ElecCreepU","V","Num","R","A2"]
[null,null,"电表工作环境","ElecPositionType",null,"Enum","R","D1","1. 户内 2. 户外 99. 其他"]
[null,null,"电表时钟准确度","ElecClockAccuracy","s/天","Num","R","A2"]
[null,null,"电表抗静电能力","ElecAntiStatic","kV","Num","R","A2"]
[null,"运行参数","电表A相电压","ElecAPhaseU","V","Inst","M","L"]
[null,null,"电表B相电压","ElecBPhaseU","V","Inst","M","L"]
[null,null,"电表C相电压","ElecCPhaseU","V","Inst","M","L"]
[null,null,"电表Uab线电压","ElecUabU","V","Inst","M","L"]
[null,null,"电表Ubc线电压","ElecUbcU","V","Inst","M","L"]
[null,null,"电表Uac线电压","ElecUacU","V","Inst","M","L"]
[null,null,"电表正序电压","ElecPositiveSequenceU","V","Inst","R","L"]
[null,null,"电表负序电压","ElecNegativeSequenceU","V","Inst","R","L"]
[null,null,"电表零序电压","ElecZeroSequenceU","V","Inst","R","L"]
[null,null,"电表A相电流","ElecAPhaseI","A","Inst","M","L"]
[null,null,"电表B相电流","ElecBPhaseI","A","Inst","M","L"]
[null,null,"电表C相电流","ElecCPhaseI","A","Inst","M","L"]
[null,null,"电表A相无功电流","ElecAPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表B相无功电流","ElecBPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表C相无功电流","ElecCPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表中性线电流","ElecNeutralI","A","Inst","R","L"]
[null,null,"电表正序电流","ElecPositiveSequenceI","A","Inst","R","L"]
[null,null,"电表负序电流","ElecNegativeSequenceI","A","Inst","R","L"]
[null,null,"电表高压零序电流","ElecHUZeroSequenceI","A","Inst","R","L"]
[null,null,"电表低压零序电流","ElecLUZeroSequenceI","A","Inst","R","L"]
[null,null,"电表频率","ElecFreq","Hz","Inst","M","L"]
[null,null,"电表A相有功功率","ElecAPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表B相有功功率","ElecBPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表C相有功功率","ElecCPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表总有功功率","ElecTotActiveP","kW","Inst","S","L"]
[null,null,"电表A相无功功率","ElecAPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表B相无功功率","ElecBPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表C相无功功率","ElecCPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表总无功功率","ElecTotReactiveP","kW","Inst","S","L"]
[null,null,"电表A相视在功功率","ElecAPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表B相视在功功率","ElecBPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表C相视在功功率","ElecCPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表总视在功功率","ElecTotApparentP","kW","Inst","S","L"]
[null,null,"电表A相功率因数","ElecAPhasePFactor",null,"Inst","R","L"]
[null,null,"电表B相功率因数","ElecBPhasePFactor",null,"Inst","R","L"]
[null,null,"电表C相功率因数","ElecCPhasePFactor",null,"Inst","R","L"]
[null,null,"电表总功率因数","ElecTotPFactor",null,"Inst","S","L"]
[null,null,"电表总谐波A相电压","ElecTotHarmonicAPhaseU","V","Inst","R","L"]
[null,null,"电表总谐波B相电压","ElecTotHarmonicBPhaseU","V","Inst","R","L"]
[null,null,"电表总谐波C相电压","ElecTotHarmonicCPhaseU","V","Inst","R","L"]
[null,null,"电表总电压谐波含量","ElecTotUHarmonic","V","Inst","M","L"]
[null,null,"电表总谐波A相电流","ElecTotHarmonicAPhaseI","A","Inst","R","L"]
[null,null,"电表总谐波B相电流","ElecTotHarmonicBPhaseI","A","Inst","R","L"]
[null,null,"电表总谐波C相电流","ElecTotHarmonicCPhaseI","A","Inst","R","L"]
[null,null,"电表总电流谐波含量","ElecTotIHarmonic","A","Inst","M","L"]
[null,null,"电表正向有功电能","ElecAccPositiveActiveE","kWh","Acc","M","L"]
[null,null,"电表反向有功电能","ElecAccReverseActiveE","kWh","Acc","M","L"]
[null,null,"电表正向无功电能","ElecAccPositiveReactiveE","kVarh","Acc","R","L"]
[null,null,"电表反向无功电能","ElecAccReverseReactiveE","kVarh","Acc","R","L"]
[null,null,"电表视在电能","ElecAccApparentE","kVAh","Acc","S","L"]
[null,null,"电表净累计有功电能","ElecNetAccActiveE","kWh","Acc","S","L"]
[null,null,"电表净累计无功电能","ElecNetAccReactiveE","kVarh","Acc","S","L"]
[null,null,"电表感性无功电能","ElecAccInductiveReactiveE","kVarh","Acc","M","L"]
[null,null,"电表容性无功电能","ElecAccCapacitiveReactiveE","kVarh","Acc","M","L"]
[null,null,"电表累计电量测量值","ElecAccConsum","kWh","Acc","S","L",null,"正向计费"]
[null,null,"电表累计金额测量值","ElecAccCost","元","Acc","S","L",null,"正向计费"]
[null,null,"电表剩余电量测量值","ElecSurplusConsum","kWh","Acc","M","L",null,"扣除计费"]
[null,null,"电表剩余金额测量值","ElecSurplusCost","元","Acc","M","L",null,"扣除计费"]
["声音传感器","技术参数-声音通用","声音传感器用途","SoundUseType",null,"Enum","S","D1","1. 测量噪声等级 2. 记录音频 99. 其他"]
[null,null,"声音传感器种类","SoundSensorType",null,"Enum","R","D1","1. 炭精粉电阻式音频传感器 2. 动圈电磁式音频传感器 3. 金属带电磁式音频传感器 4. 薄膜电容式音频传感器 5. 驻极体电容式音频传感器 6. 压电陶瓷式音频传感器 7. 激光反射式音频传感器 99. 其他"]
[null,"技术参数-噪声传感器","噪声声强测量上限","SoundNoiseUpperDBLimit","dB(A)","Num","M","A2"]
[null,null,"噪声声强测量下限","SoundNoiseLowerDBLimit","dB(A)","Num","M","A2"]
[null,null,"噪声频率测量上限","SoundNoiseUpperFreqLimit","Hz","Num","M","A2"]
[null,null,"噪声频率测量下限","SoundNoiseLowerFreqLimit","Hz","Num","M","A2"]
[null,null,"噪声传感器传递函数","SoundNoiseTransFunc",null,"Str","R","B1"]
[null,null,"噪声传感器频率加权特性","SoundNoiseFreqWeightCharacter",null,"MEnum","R","D2","1. A 2. B 3. C 99. 其他 （可多选）"]
[null,null,"噪声传感器加权动态测量范围","SoundNoiseWeightMeasureRange","dB(A)","Num","R","A6"]
[null,"技术参数-录音","录音传感器录制格式","SoundAudioRecordFormat",null,"MEnum","M","D2","1. MP3 2. WAV 3. WMA 4. ACC 99. 其他 （可多选）"]
[null,null,"录音传感器连续录制时间","SoundAudioContinueRecordTime","h","Num","M","A2"]
[null,null,"录音传感器信噪比下限","SoundAudioSNRLowerLimit","dB(A)","Num","R","A2"]
[null,null,"录音传感器失真度上限","SoundAudioDistortionUpperLimit","%","Num","R","A2"]
[null,"运行参数","噪声传感器声强测量值","SoundNoise","dB(A)","Inst","S","L"]
[null,null,"录音传感器是否录制音频","isSoundAudioRecord",null,"Boolv","S","L","0. 否 1. 是"]
[null,null,"录音传感器音频地址","SoundAudioAddress",null,"Strv","S","L"]
["图像传感器","技术参数","图像传感器敏感元器件种类","ImageSensorType",null,"Enum","R","D1","1. CCD 2. CMOS 99. 其他"]
[null,null,"图像传感器色彩类型","ImageColorType",null,"Enum","S","D1","1. 黑白 2. 彩色 99. 其他"]
[null,null,"图像传感器是否有自动调焦功能","isImageAutoFocusFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器是否能俯仰","isImagePitch",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器俯仰速度","ImagePitchSpeed","°/s","Num","R","A2"]
[null,null,"图像传感器是否能旋转","isImageRotate",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器旋转速度","ImageRotateSpeed","°/s","Num","R","A2"]
[null,null,"图像传感器最大焦距","ImageMaxFocalDistance","mm","Num","R","A2"]
[null,null,"图像传感器最小焦距","ImageMinFocalDistance","mm","Num","R","A2"]
[null,null,"图像传感器视野","ImageViewAngle","°","Num","R","A2"]
[null,null,"图像传感器最大光圈","ImageMaxAperture",null,"Num","R","A1"]
[null,null,"图像传感器最小光圈","ImageMinAperture",null,"Num","R","A1"]
[null,null,"图像传感器水平像素个数","ImageHorizontalPixelNum","个","Num","R","A2"]
[null,null,"图像传感器垂直像素个数","ImageVerticalPixelNum","个","Num","R","A2"]
[null,null,"图像传感器曝光时间","ImageExposureTime","s","Num","R","A2"]
[null,null,"图像传感器是否有辅助光源","isImageAuxiliaryLight",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器亮灯方式","ImageLightType",null,"Enum","R","D1","1. 脉冲亮灯 2. DC亮灯 99. 其他"]
[null,null,"图像传感器有无图像识别功能","isImageRecognizeFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"图像传感器延迟时间","ImageDelayTime","s","Num","R","A2"]
[null,null,"图像传感器录制视频格式","ImageRecordFormat",null,"MEnum","M","D2","1. MPEG/MPG/DAT 2. AVI 3. MOV 4. ASF 5. WMV 6. NAVI 7. 3GP 8. REAL VIDEO 9. MKV 10. FLV 11. F4V 12. RMVB 13. WebM 14. HDDVD 15. Blu-ray 16. qsv 99. 其他 （可多选）"]
[null,null,"图像传感器连续录制时间","ImageContinueRecordTime","h","Num","M","A2"]
[null,null,"图像传感器抗震动","ImageAntiVibration",null,"Str","R","B1",null,"eg:10至55Hz双向振幅1.5mmXYZ各方向2个小时"]
[null,null,"图像传感器抗冲击","ImageAntiImpact",null,"Str","R","B1",null,"eg:500m/s26个方向各3次"]
[null,null,"图像传感器控制模式","ImageCtrlType",null,"MEnum","R","D2","1. 外部触发 2. 程序切换 3. 错误区域 4. 外部标准图像注册 5. 辅助光源开关 99. 其他 （可多选）"]
[null,"运行参数","图像传感器是否输出视频","isImageRecord",null,"Boolv","S","L","0. 否 1. 是"]
[null,null,"图像传感器输出视频地址","ImageAddress",null,"Strv","S","L"]
["人流量传感器","技术参数","原理类型",null,null,"Enum","R","D1","1. 红外光电式 2. 多摄像头立体视觉式 3. 单摄像头式 4. RFID式 5. 移动设备式 99. 其他"]
[null,null,"用途类型",null,null,"MEnum","S","D2","1. 计量人流量 2. 监测室内人数 3. 人员位置监控 4. 入侵探测 99. 其他 （可多选）"]
[null,null,"是否有方向性",null,null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"是否特定人群",null,null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否能同时计量多人",null,null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"记录方式",null,null,"Enum","R","D1","1. 逐时记录 2. 记录改变量 3. 累计计数 99. 其他"]
[null,"运行参数","是否有人通过/靠近",null,null,"Enumv","S","L"," -1. 负向通过 0. 无 1. 正向通过/有人靠近"]
[null,null,"正向累计流量",null,"人次","Inst","M","L"]
[null,null,"负向累计流量",null,"人次","Inst","M","L"]
[null,null,"室内人数",null,"人","Inst","R","L"]
[null,null,"人员位置",null,null,"Attachmentv","R","L"]

{"sheet":"SETP温度传感器","index":1,"n_rows":91,"n_cols":10,"rows_kept":91,"cut":false,"hidden":false,"merged":[[0,0,0,9],[46,0,47,1],[48,0,90,0],[48,1,51,1],[52,1,55,1],[56,1,58,1],[59,1,61,1],[62,1,71,1],[72,1,74,1],[75,1,78,1],[79,1,87,1],[88,1,90,1],[1,0,1,1],[2,0,45,1]]}
["温度传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["温度传感器","技术参数-温度通用","温度传感器种类","TempSensorType",null,"Enum","R","D1","1. 热电偶温度传感器 2. 热敏电阻温度传感器 3. 电阻温度传感器 4. IC温度传感器 5. 玻璃管温度计 6. 压力式温度计 7. 红外光电测温仪 8. 热色液晶测温仪 9. 全息干涉技术测温 99. 其他"]
[null,null,"温度测量上限","TempUpperLimit","℃","Num","M","A2"]
[null,null,"温度测量下限","TempLowerLimit","℃","Num","M","A2"]
[null,null,"温度传感器传递函数","TempTransFunc",null,"Str","R","B1"]
[null,"技术参数-热电偶温度传感器","热电偶温度传感器分度号","TempThermocoupleGraduation",null,"Enum","R","D1","1. S 2. R 3. B 4. N 5. K 6. E 7. J 8. T 99. 其他","不同的分度号表示不同的材料"]
[null,null,"热电偶温度传感器布置方式","TempThermocoupleInstallType",null,"Enum","R","D1","1. 触壁式 2. 非触壁式 3. 暴露式 99. 其他"]
[null,null,"热电偶温度传感器结构形式","TempThermocoupleStructureType",null,"Enum","R","D1","1. 普通热电偶 2. 耐磨热电偶 3. 铠装热电偶 4. 防爆热电偶 99. 其他"]
[null,null,"热电偶温度传感器插入深度","TempThermocoupleInsertDepth","mm","Num","R","A2"]
[null,"技术参数-热敏电阻温度传感器","热敏电阻温度传感器材料类型","TempThermistorMaterial",null,"Enum","R","D1","1. PTC 2. RTC 99. 其他"]
[null,null,"热敏电阻温度传感器电阻标称值","TempThermistorResistance","Ω","Num","R","A2"]
[null,null,"热敏电阻温度传感器耗散系数","TempThermistorDissipationCoeff","mW/℃","Num","R","A2"]
[null,"技术参数-电阻温度传感器","电阻温度传感器材料","TempResistorMaterial",null,"Enum","R","D1","1. 铂 2. 铜 3. 镍4. 铁镍合金 99. 其他"]
[null,null,"电阻温度传感器标称值","TempResistorResistance","Ω","Num","R","A2",null,"0℃时的电阻"]
[null,null,"电阻温度传感器耗散系数","TempResistorDissipationCoeff","mW/℃","Num","R","A2"]
[null,"技术参数-IC温度传感器","IC温度传感器种类","TempICSensorType",null,"Bool","R","E1","0. 模拟IC温度传感器 1. 数字IC温度传感器"]
[null,null,"IC温度传感器AD转换位数","TempICADConverseBit","bit","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器标称频率","TempICFreq","Hz","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出PWM低电压","TempICOutPWMLowU","V","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出PWM高电压","TempICOutPWMHighU","V","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器上升时间","TempICRiseTime","μs","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器下降时间","TempICFallTime","μs","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器电源抑制比","TempICPSRR","dB(A)","Num","R","A2",null,"数字"]
[null,null,"IC温度传感器输出增益","TempICOutGain","dB(A)","Num","R","A2",null,"模拟"]
[null,null,"IC温度传感器0℃输出偏移","TempICOutOffset","mV","Num","R","A2",null,"模拟"]
[null,"技术参数-玻璃管式温度计","玻璃管温度传感器内部液体种类","TempTubeLiquidType",null,"Enum","R","D1","1. 水银 2. 有机液体 99. 其他"]
[null,null,"玻璃管温度传感器内部长度","TempTubeLength","mm","Num","R","A2"]
[null,null,"玻璃管温度传感器内部直径","TempTubeDiameter","mm","Num","R","A2"]
[null,"技术参数-压力式温度计","压力式温度传感器尾部长度","TempPressTailLength","mm","Num","R","A2"]
[null,null,"压力式温度传感器温包材料","TempPressBulbMaterial",null,"Enum","R","D1","1. 铜 2. 不锈钢 99. 其他"]
[null,null,"压力式温度传感器毛细管材料","TempPressCapillaryMaterial",null,"Enum","R","D1","1. 铜 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"压力式温度传感器温包插入深度范围","TempPressInsertDepthRange","mm","Num","R","A6"]
[null,"技术参数-红外测温仪","红外温度传感器探测器类型","TempInfraredDetectorType",null,"Bool","R","E1","0. 非制冷红外焦平面 1. 制冷红外焦平面"]
[null,null,"红外温度传感器探测元数量","TempInfraredDetectorNum",null,"Num","R","A3",null,"eg：160*220分别代表长宽方向的探测元数量"]
[null,null,"红外温度传感器响应波段","TempInfraredResponseBand","μm","Num","R","A2"]
[null,null,"红外温度传感器焦距","TempInfraredFocalDistance","mm","Num","R","A2"]
[null,null,"红外温度传感器NETD","TempInfraredNETD","mK","Num","R","A2"]
[null,null,"红外温度传感器IFOV","TempInfraredIFOV","mrad","Num","R","A2"]
[null,null,"红外温度传感器视场角","TempInfraredFieldAngle","°","Num","R","A4",null,"eg：3.6˚*1.2˚"]
[null,null,"红外温度传感器是否有自动调焦功能","isTempInfraredAutoFocusFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"红外温度传感器显示图像模式","TempInfraredDisplayType",null,"Enum","R","D1","1. 红外 2. 可见光 3. MIF 4. PIP 99. 其他"]
[null,"运行参数","温度传感器输出电压","TempOutU","V","Inst","R","L"]
[null,null,"温度传感器输出电流","TempOutI","A","Inst","R","L"]
[null,null,"温度传感器温度测量值","Temp","℃","Inst","S","L"]

{"sheet":"SERH湿度传感器","index":2,"n_rows":58,"n_cols":10,"rows_kept":58,"cut":false,"hidden":false,"merged":[[48,0,57,0],[48,1,54,1],[55,1,57,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["湿度传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["湿度传感器","技术参数","湿度传感器种类","RHSensorType",null,"Enum","R","D1","1. 电解质湿度传感器 2. MOS陶瓷湿度传感器 3. 高分子湿度传感器 4. 热敏电阻式湿度传感器 5. 红外吸收式湿度传感器 6. 微波式湿度传感器 7. 超声波湿度传感器 99. 其他"]
[null,null,"湿度测量上限","RHUpperLimit","%RH","Num","M","A2"]
[null,null,"湿度测量下限","RHLowerLimit","%RH","Num","M","A2"]
[null,null,"湿度传感器传递函数","RHTransFunc",null,"Str","R","B1"]
[null,null,"湿度传感器湿滞回差","RHHysteresisReturnDifference",null,"Num","R","A1"]
[null,null,"湿度传感器温度系数","RHTempCoeff","%RH/℃","Num","R","A2"]
[null,null,"湿度传感器外壳材料","RHShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,"运行参数","湿度传感器输出电压","RHOutU","V","Inst","R","L"]
[null,null,"湿度传感器输出电流","RHOutI","A","Inst","R","L"]
[null,null,"湿度传感器相对湿度测量值","RH","%RH","Inst","S","L"]

{"sheet":"SEPS压力传感器","index":3,"n_rows":62,"n_cols":10,"rows_kept":62,"cut":false,"hidden":false,"merged":[[48,0,61,0],[48,1,58,1],[59,1,61,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["压力传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["压力传感器","技术参数","压力传感器种类","PressSensorType",null,"Enum","R","D1","1. 液柱式压力计 1.1 U形管压力计 1.2 斜管微压计 1.3 单管压力计 2. 弹性压力计 2.1 膜片压力计 2.1.1 电容式压力传感器 2.1.2 光纤式压力传感器 2.1.3 力矩平衡式压力变送器 2.2 弹簧管 2.2.1 弹簧管压力表 2.2.2 霍尔远传压力表 2.3 波纹管 3. 电气式压力计 3.1 压电式压力传感器 3.2 应变式压力传感器 3.3 压阻式压力传感器 4. 负荷式压力计 4.1 活塞式压力计 4.2 钟罩式微压计 99. 其他"]
[null,null,"压力传感器介质","PressMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 2. 液体\n2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）"]
[null,null,"压力测量上限","PressUpperLimit","Pa","Num","M","A2"]
[null,null,"压力测量下限","PressLowerLimit","Pa","Num","M","A2"]
[null,null,"压力传感器传递函数","PressTransFunc",null,"Str","R","B1"]
[null,null,"压力传感器温度补偿","PressTempCompensation","℃","Num","R","A2"]
[null,null,"压力传感器负载电阻","PressLoadResistance","Ω","Num","R","A2"]
[null,null,"压力传感器绝缘电阻","PressInsulationResistance","Ω","Num","R","A2"]
[null,null,"压力传感器输出负载","PressOutLoad","Ω","Num","R","A2"]
[null,null,"压力传感器温漂系数","PressTempDriftCoeff","mm","Num","R","A2"]
[null,null,"压力传感器外壳材料","PressShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,"运行参数","压力传感器输出电压","PressOutU","V","Inst","R","L"]
[null,null,"压力传感器输出电流","PressOutI","A","Inst","R","L"]
[null,null,"压力传感器压力测量值","Press","Pa","Inst","S","L"]

{"sheet":"SECT浓度传感器","index":4,"n_rows":64,"n_cols":10,"rows_kept":64,"cut":false,"hidden":false,"merged":[[48,0,63,0],[48,1,58,1],[59,1,63,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["浓度传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["浓度传感器","技术参数","浓度传感器测量对象","ConcentrateSensorType",null,"MEnum","S","D2","1. 一氧化碳 2. 二氧化碳 3. 二氧化硫 4. 氮氧化物 5. 甲醛 6. 苯 7. 总挥发性有机化合物 8. 总悬浮颗粒 9. 可吸入颗粒物 10. 烟雾浓度 11. 生物微粒 12. 水硬度 13. PH值 14. SS值 15. COD值 99. 其他 （可多选）","硬度：水总硬度是指水中Ca2+、Mg2+的总量；SS值：水中悬浮物；COD值：化学需氧量，是在一定的条件下，采用一定的强氧化剂处理水样时，所消耗的氧气的量，表示水中还原性物质多少"]
[null,null,"浓度传感器介质种类","ConcentrateMediumType",null,"Enum","M","D1","1. 气体 2. 液体 99. 其他"]
[null,null,"浓度传感器是否有报警功能","isAlarmFunc",null,"Bool","S","E1","0. 否  1. 是"]
[null,null,"浓度传感器最大报警电流","MaxAlarmI","A","Num","R","A2"]
[null,null,"浓度测量上限","ConcentrateUpperLimit",null,"Num","M","A1"]
[null,null,"浓度测量下限","ConcentrateLowerLimit",null,"Num","M","A1"]
[null,null,"浓度测量单位类型","ConcentrateMeasureUnitType",null,"MEnum","S","D2","1. ppm 2. μg/m3 3. μg/L 4. mmol/L 99. 其他 （多选）","液、气体中的气体ppm；气体中的颗粒物μg/m3；液体中的悬浮物ug/L；液体中离子mmol/L"]
[null,null,"浓度传感器传递函数","ConcentrateTransFunc",null,"Str","R","B1"]
[null,null,"浓度传感器外壳材料","ConcentrateShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"浓度传感器采样流量","ConcentrateSampleFlow","mL/min","Num","R","A2"]
[null,null,"浓度传感器采样方式","ConcentrateSampleMode",null,"Str","R","B1"]
[null,"运行参数","浓度传感器是否正在报警","isConcentrateAlarm",null,"Boolv","S","L","0. 否  1. 是"]
[null,null,"浓度传感器输出电压","ConcentrateOutU","V","Inst","R","L"]
[null,null,"浓度传感器输出电流","ConcentrateOutI","A","Inst","R","L"]
[null,null,"浓度传感器浓度测量单位","ConcentrateUnit",null,"Enumv","S","D1","1. ppm 2. μg/m3 3. μg/L 4. mmol/L 99. 其他"]
[null,null,"浓度传感器浓度测量值","Concentrate",null,"Inst","S","L"]

{"sheet":"SESP速度传感器","index":5,"n_rows":57,"n_cols":10,"rows_kept":57,"cut":false,"hidden":false,"merged":[[48,0,56,0],[48,1,53,1],[54,1,56,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["速度传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["速度传感器","技术参数","速度传感器原理类型","VSensorType",null,"Enum","R","D1","1. 机械式风速仪 2. 热线风速仪 3. 测压管 4. 激光多普勒测速仪 99. 其他"]
[null,null,"速度传感器介质种类","VMediumType",null,"Enum","S","D1","1. 气体 2. 液体 99. 其他"]
[null,null,"速度传感器外壳材料","VShellMaterial",null,"Enum","R","D1","1. 铝合金 2. 不锈钢 3. 塑料 99. 其他"]
[null,null,"速度测量上限","VUpperLimit","m/s","Num","M","A2"]
[null,null,"速度测量下限","VLowerLimit","m/s","Num","M","A2"]
[null,null,"速度传感器传递函数","VTransFunc",null,"Str","R","B1"]
[null,"运行参数","速度传感器输出电压","VOutU","V","Inst","R","L"]
[null,null,"速度传感器输出电流","VOutI","A","Inst","R","L"]
[null,null,"速度传感器速度测量值","V","m/s","Inst","S","L"]

{"sheet":"SEDP位移传感器","index":6,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[48,0,60,0],[48,1,57,1],[58,1,60,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["位移传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["位移传感器","技术参数","位移传感器原理类型","DisplaceSensorType",null,"Enum","R","D1","1. 金属膜 2. 导电塑料 3. 光电式 4. 磁敏式 5. 金属玻璃轴 6. 绕线式 7. 数字激光式 99. 其他","应用领域：自动门（列车及大厅）；拉绳/拉线；电梯平层；升降机；开关窗记录仪"]
[null,null,"位移传感器传递函数","DisplaceTransFunc",null,"Str","R","B1"]
[null,null,"位移测量上限","DisplaceUpperLimit","mm","Num","M","A2"]
[null,null,"位移测量下限","DisplaceLowerLimit","mm","Num","M","A2"]
[null,null,"位移传感器标称电阻","DisplaceResistance","kΩ","Num","R","A2"]
[null,null,"位移传感器阻值公差","DisplaceResistanceTolerance","%","Num","R","A2"]
[null,null,"位移传感器绝缘电阻","DisplaceInsulationResistance","MΩ","Num","R","A2"]
[null,null,"位移传感器绝缘强度","DisplaceInsulationStrength","kV/mm","Num","R","A2"]
[null,null,"位移传感器振动","DisplaceVibration","Hz","Num","R","A2"]
[null,null,"位移传感器驱动力（水平方向）","DisplaceDriveForce ","N","Num","R","A2"]
[null,"运行参数","位移传感器输出电压","DisplaceOutU","V","Inst","R","L"]
[null,null,"位移传感器输出电流","DisplaceOutI","A","Inst","R","L"]
[null,null,"位移传感器位移测量值","Displace","m ","Inst","S","L"]

{"sheet":"SEFL流量传感器","index":7,"n_rows":65,"n_cols":10,"rows_kept":65,"cut":false,"hidden":false,"merged":[[48,0,64,0],[48,1,56,1],[57,1,64,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["流量传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["流量传感器","技术参数","流量传感器原理类型","FlowSensorType",null,"Enum","R","D1","1. 压差式 1.1 孔板流量计 1.2 喷嘴 1.3 文丘利管 1.4 V形内锥式流量计 1.5 转子流量计 1.6 动压平均管 2. 叶轮式 2.1 水表 2.2 涡轮流量计 3. 电磁流量计 4. 超声波流量计 5. 涡街流量计 6. 容积流量计 6.1 腰轮流量计 6.2 转式气体流量计 6.3 薄膜式气体流量计 99. 其他"]
[null,null,"流量传感器介质种类","FlowMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 1.5 蒸汽 2. 液体 2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）"]
[null,null,"流量测量上限","FlowUpperLimit",null,"Num","M","A2"]
[null,null,"流量测量下限","FlowLowerLimit",null,"Num","M","A2"]
[null,null,"流量测量单位类型","FlowMeasureUnitType",null,"MEnum","S","D2","1. kg/h 2. m3/s 3. kgf/h 99. 其他 （多选）"]
[null,null,"流量传感器传递函数","FlowTransFunc",null,"Str","R","B1"]
[null,null,"流量传感器内部电容","FlowInElecCap","pF","Num","R","A2"]
[null,null,"流量传感器温度变化响应时间","FlowTempResponseTime","s","Num","R","A2"]
[null,null,"流量传感器温度梯度","FlowTempGradient","℃/min","Num","R","A2"]
[null,"运行参数","流量传感器输出电压","FlowOutU","V","Inst","R","L"]
[null,null,"流量传感器输出电流","FlowOutI","A","Inst","R","L"]
[null,null,"流量传感器流速测量值","FlowSpeed","m/s","Inst","M","L"]
[null,null,"流量传感器流量测量值","Flow","m3/h","Inst","S","L"]
[null,null,"流量传感器累计流量测量值","FlowAccVolume","m3","Acc","M","L",null,"正向计费"]
[null,null,"流量传感器累计金额测量值","FlowAccCost","元","Acc","M","L",null,"正向计费"]
[null,null,"流量传感器剩余流量测量值","FlowSurplusVolume","m3","Acc","M","L",null,"扣除计费"]
[null,null,"流量传感器剩余金额测量值","FlowSurplusCost","元","Acc","M","L",null,"扣除计费"]

{"sheet":"SEHT热量传感器","index":8,"n_rows":71,"n_cols":10,"rows_kept":71,"cut":false,"hidden":false,"merged":[[48,0,70,0],[48,1,60,1],[61,1,70,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["热量传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["热量传感器","技术参数","热量传感器功能类型","HeatFuncType",null,"Enum","M","D1","1. 流体单热量表 2. 流体冷热量表 3. 热流密度计 99. 其他"]
[null,null,"热量传感器原理类型","HeatPrincipleType",null,"Enum","R","D1","1. 机械式热量表 2. 超声波式热量表 3. 电磁式热量表 99. 其他","流体量表"]
[null,null,"热量传感器结构类型","HeatStructType",null,"Enum","R","D1","1. 整体式热量表 2. 组合式热量表 3. 紧凑式热量表 99. 其他","流体量表"]
[null,null,"热量传感器功率类型","HeatPowerType",null,"Enum","R","D1","1. 户用量表（DN≤40mm） 2. 工业用量表（DN>40mm） 99. 其他","流体量表"]
[null,null,"热量传感器精度等级","HeatPrecisionType",null,"Enum","R","D1","1. 一级表 2. 二级表 3. 三级表 99. 其他","流体量表"]
[null,null,"热量传感器介质种类","HeatMediumType",null,"MEnum","S","D2","1. 气体 1.1 空气 1.2 燃气 1.3 烟气 1.4 煤气 2. 液体\n2.1 水 2.2 制冷剂 2.3 油 99. 其他 （可多选）","流体量表"]
[null,null,"热量传感器热传递类型","HeatTransType",null,"MEnum","R","D2","1. 热传导 2. 热辐射 3. 热对流 99. 其他 （可多选）","热流计"]
[null,null,"热量传感器数量类型","HeatSensorNumType",null,"Bool","R","E1","0. 单通道热流计 1. 多通道热流计","热流计"]
[null,null,"热量传感器外形类型","HeatShapeType",null,"Enum","R","D1","1. 手持式热流计 2. 便携式热流计 99. 其他","热流计"]
[null,null,"热（流）量测量上限","HeatUpperLimit","kW/m2","Num","M","A2"]
[null,null,"热（流）量测量下限","HeatLowerLimit","kW/m2","Num","M","A2"]
[null,null,"热量传感器传递函数","HeatTransFunc",null,"Str","R","B1"]
[null,null,"热量传感器响应时间","HeatResponseTime","s","Num","R","A2"]
[null,"运行参数","热量传感器输出电压","HeatOutU","V","Inst","R","L"]
[null,null,"热量传感器输出电流","HeatOutI","A","Inst","R","L"]
[null,null,"热量传感器温差测量值","HeatTempDifference","℃","Inst","M","L",null,"流体量表"]
[null,null,"热量传感器流量测量值","HeatFlow","m3/h","Inst","M","L",null,"流体量表"]
[null,null,"热量传感器热量测量值","Heat","kW","Inst","S","L"]
[null,null,"热量传感器热流量测量值","HeatIndensity","kW/m2","Inst","S","L"]
[null,null,"热量传感器累计热量测量值","HeatAccHeat","kWh","Acc","M","L",null,"正向计费"]
[null,null,"热量传感器累计金额测量值","HeatAccCost","元","Acc","M","L",null,"正向计费"]
[null,null,"热量传感器剩余热量测量值","HeatSurplusHeat","kWh","Acc","M","L",null,"扣除计费"]
[null,null,"热量传感器剩余金额测量值","HeatSurplusCost","元","Acc","M","L",null,"扣除计费"]

{"sheet":"SEEE电度传感器","index":9,"n_rows":119,"n_cols":10,"rows_kept":119,"cut":false,"hidden":false,"merged":[[48,0,118,0],[48,1,60,1],[61,1,118,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["电度传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["电度传感器","技术参数","电表种类","ElecMeterType",null,"Enum","S","D1","1. 单向电能表 2. 三相三线电能表 3. 三相四线电能表 4. 综保电表 5. 计费电表 99. 其他"]
[null,null,"电表准确度等级","ElecAccuracyLev",null,"Enum","R","D1","1. 1级 2. 2级 99. 其他"]
[null,null,"电表是否有多费率功能","isElecMultiRateFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"电表是否有预付费功能","isElecPrepayFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"电表PT变比","ElecPTRatio",null,"Num","M","A1"]
[null,null,"电表CT变比","ElecCTRatio",null,"Num","M","A1"]
[null,null,"电表标准参比电压","ElecRatedRefU","V","Num","R","A2"]
[null,null,"电表标准参比频率","ElecRatedRefFreq","Hz","Num","R","A2"]
[null,null,"电表最大电流","ElecMaxI","A","Num","R","A2"]
[null,null,"电表潜动电压","ElecCreepU","V","Num","R","A2"]
[null,null,"电表工作环境","ElecPositionType",null,"Enum","R","D1","1. 户内 2. 户外 99. 其他"]
[null,null,"电表时钟准确度","ElecClockAccuracy","s/天","Num","R","A2"]
[null,null,"电表抗静电能力","ElecAntiStatic","kV","Num","R","A2"]
[null,"运行参数","电表A相电压","ElecAPhaseU","V","Inst","M","L"]
[null,null,"电表B相电压","ElecBPhaseU","V","Inst","M","L"]
[null,null,"电表C相电压","ElecCPhaseU","V","Inst","M","L"]
[null,null,"电表Uab线电压","ElecUabU","V","Inst","M","L"]
[null,null,"电表Ubc线电压","ElecUbcU","V","Inst","M","L"]
[null,null,"电表Uac线电压","ElecUacU","V","Inst","M","L"]
[null,null,"电表正序电压","ElecPositiveSequenceU","V","Inst","R","L"]
[null,null,"电表负序电压","ElecNegativeSequenceU","V","Inst","R","L"]
[null,null,"电表零序电压","ElecZeroSequenceU","V","Inst","R","L"]
[null,null,"电表A相电流","ElecAPhaseI","A","Inst","M","L"]
[null,null,"电表B相电流","ElecBPhaseI","A","Inst","M","L"]
[null,null,"电表C相电流","ElecCPhaseI","A","Inst","M","L"]
[null,null,"电表A相无功电流","ElecAPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表B相无功电流","ElecBPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表C相无功电流","ElecCPhaseReactiveI","A","Inst","R","L"]
[null,null,"电表中性线电流","ElecNeutralI","A","Inst","R","L"]
[null,null,"电表正序电流","ElecPositiveSequenceI","A","Inst","R","L"]
[null,null,"电表负序电流","ElecNegativeSequenceI","A","Inst","R","L"]
[null,null,"电表高压零序电流","ElecHUZeroSequenceI","A","Inst","R","L"]
[null,null,"电表低压零序电流","ElecLUZeroSequenceI","A","Inst","R","L"]
[null,null,"电表频率","ElecFreq","Hz","Inst","M","L"]
[null,null,"电表A相有功功率","ElecAPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表B相有功功率","ElecBPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表C相有功功率","ElecCPhaseActiveP","kW","Inst","M","L"]
[null,null,"电表总有功功率","ElecTotActiveP","kW","Inst","S","L"]
[null,null,"电表A相无功功率","ElecAPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表B相无功功率","ElecBPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表C相无功功率","ElecCPhaseReactiveP","kW","Inst","M","L"]
[null,null,"电表总无功功率","ElecTotReactiveP","kW","Inst","S","L"]
[null,null,"电表A相视在功功率","ElecAPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表B相视在功功率","ElecBPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表C相视在功功率","ElecCPhaseApparentP","kW","Inst","R","L"]
[null,null,"电表总视在功功率","ElecTotApparentP","kW","Inst","S","L"]
[null,null,"电表A相功率因数","ElecAPhasePFactor",null,"Inst","R","L"]
[null,null,"电表B相功率因数","ElecBPhasePFactor",null,"Inst","R","L"]
[null,null,"电表C相功率因数","ElecCPhasePFactor",null,"Inst","R","L"]
[null,null,"电表总功率因数","ElecTotPFactor",null,"Inst","S","L"]
[null,null,"电表总谐波A相电压","ElecTotHarmonicAPhaseU","V","Inst","R","L"]
[null,null,"电表总谐波B相电压","ElecTotHarmonicBPhaseU","V","Inst","R","L"]
[null,null,"电表总谐波C相电压","ElecTotHarmonicCPhaseU","V","Inst","R","L"]
[null,null,"电表总电压谐波含量","ElecTotUHarmonic","V","Inst","M","L"]
[null,null,"电表总谐波A相电流","ElecTotHarmonicAPhaseI","A","Inst","R","L"]
[null,null,"电表总谐波B相电流","ElecTotHarmonicBPhaseI","A","Inst","R","L"]
[null,null,"电表总谐波C相电流","ElecTotHarmonicCPhaseI","A","Inst","R","L"]
[null,null,"电表总电流谐波含量","ElecTotIHarmonic","A","Inst","M","L"]
[null,null,"电表正向有功电能","ElecAccPositiveActiveE","kWh","Acc","M","L"]
[null,null,"电表反向有功电能","ElecAccReverseActiveE","kWh","Acc","M","L"]
[null,null,"电表正向无功电能","ElecAccPositiveReactiveE","kVarh","Acc","R","L"]
[null,null,"电表反向无功电能","ElecAccReverseReactiveE","kVarh","Acc","R","L"]
[null,null,"电表视在电能","ElecAccApparentE","kVAh","Acc","S","L"]
[null,null,"电表净累计有功电能","ElecNetAccActiveE","kWh","Acc","S","L"]
[null,null,"电表净累计无功电能","ElecNetAccReactiveE","kVarh","Acc","S","L"]
[null,null,"电表感性无功电能","ElecAccInductiveReactiveE","kVarh","Acc","M","L"]
[null,null,"电表容性无功电能","ElecAccCapacitiveReactiveE","kVarh","Acc","M","L"]
[null,null,"电表累计电量测量值","ElecAccConsum","kWh","Acc","S","L",null,"正向计费"]
[null,null,"电表累计金额测量值","ElecAccCost","元","Acc","S","L",null,"正向计费"]
[null,null,"电表剩余电量测量值","ElecSurplusConsum","kWh","Acc","M","L",null,"扣除计费"]
[null,null,"电表剩余金额测量值","ElecSurplusCost","元","Acc","M","L",null,"扣除计费"]

{"sheet":"SESD声音传感器","index":10,"n_rows":64,"n_cols":10,"rows_kept":64,"cut":false,"hidden":false,"merged":[[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1],[48,0,63,0],[48,1,49,1],[50,1,56,1],[57,1,60,1],[61,1,63,1]]}
["声音传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["声音传感器","技术参数-声音通用","声音传感器用途","SoundUseType",null,"Enum","S","D1","1. 测量噪声等级 2. 记录音频 99. 其他"]
[null,null,"声音传感器种类","SoundSensorType",null,"Enum","R","D1","1. 炭精粉电阻式音频传感器 2. 动圈电磁式音频传感器 3. 金属带电磁式音频传感器 4. 薄膜电容式音频传感器 5. 驻极体电容式音频传感器 6. 压电陶瓷式音频传感器 7. 激光反射式音频传感器 99. 其他"]
[null,"技术参数-噪声传感器","噪声声强测量上限","SoundNoiseUpperDBLimit","dB(A)","Num","M","A2"]
[null,null,"噪声声强测量下限","SoundNoiseLowerDBLimit","dB(A)","Num","M","A2"]
[null,null,"噪声频率测量上限","SoundNoiseUpperFreqLimit","Hz","Num","M","A2"]
[null,null,"噪声频率测量下限","SoundNoiseLowerFreqLimit","Hz","Num","M","A2"]
[null,null,"噪声传感器传递函数","SoundNoiseTransFunc",null,"Str","R","B1"]
[null,null,"噪声传感器频率加权特性","SoundNoiseFreqWeightCharacter",null,"MEnum","R","D2","1. A 2. B 3. C 99. 其他 （可多选）"]
[null,null,"噪声传感器加权动态测量范围","SoundNoiseWeightMeasureRange","dB(A)","Num","R","A6"]
[null,"技术参数-录音","录音传感器录制格式","SoundAudioRecordFormat",null,"MEnum","M","D2","1. MP3 2. WAV 3. WMA 4. ACC 99. 其他 （可多选）"]
[null,null,"录音传感器连续录制时间","SoundAudioContinueRecordTime","h","Num","M","A2"]
[null,null,"录音传感器信噪比下限","SoundAudioSNRLowerLimit","dB(A)","Num","R","A2"]
[null,null,"录音传感器失真度上限","SoundAudioDistortionUpperLimit","%","Num","R","A2"]
[null,"运行参数","噪声传感器声强测量值","SoundNoise","dB(A)","Inst","S","L"]
[null,null,"录音传感器是否录制音频","isSoundAudioRecord",null,"Boolv","S","L","0. 否 1. 是"]
[null,null,"录音传感器音频地址","SoundAudioAddress",null,"Strv","S","L"]

{"sheet":"SEVD图像传感器","index":11,"n_rows":74,"n_cols":10,"rows_kept":74,"cut":false,"hidden":false,"merged":[[48,0,73,0],[48,1,71,1],[72,1,73,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["图像传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["图像传感器","技术参数","图像传感器敏感元器件种类","ImageSensorType",null,"Enum","R","D1","1. CCD 2. CMOS 99. 其他"]
[null,null,"图像传感器色彩类型","ImageColorType",null,"Enum","S","D1","1. 黑白 2. 彩色 99. 其他"]
[null,null,"图像传感器是否有自动调焦功能","isImageAutoFocusFunc",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器是否能俯仰","isImagePitch",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器俯仰速度","ImagePitchSpeed","°/s","Num","R","A2"]
[null,null,"图像传感器是否能旋转","isImageRotate",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器旋转速度","ImageRotateSpeed","°/s","Num","R","A2"]
[null,null,"图像传感器最大焦距","ImageMaxFocalDistance","mm","Num","R","A2"]
[null,null,"图像传感器最小焦距","ImageMinFocalDistance","mm","Num","R","A2"]
[null,null,"图像传感器视野","ImageViewAngle","°","Num","R","A2"]
[null,null,"图像传感器最大光圈","ImageMaxAperture",null,"Num","R","A1"]
[null,null,"图像传感器最小光圈","ImageMinAperture",null,"Num","R","A1"]
[null,null,"图像传感器水平像素个数","ImageHorizontalPixelNum","个","Num","R","A2"]
[null,null,"图像传感器垂直像素个数","ImageVerticalPixelNum","个","Num","R","A2"]
[null,null,"图像传感器曝光时间","ImageExposureTime","s","Num","R","A2"]
[null,null,"图像传感器是否有辅助光源","isImageAuxiliaryLight",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"图像传感器亮灯方式","ImageLightType",null,"Enum","R","D1","1. 脉冲亮灯 2. DC亮灯 99. 其他"]
[null,null,"图像传感器有无图像识别功能","isImageRecognizeFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"图像传感器延迟时间","ImageDelayTime","s","Num","R","A2"]
[null,null,"图像传感器录制视频格式","ImageRecordFormat",null,"MEnum","M","D2","1. MPEG/MPG/DAT 2. AVI 3. MOV 4. ASF 5. WMV 6. NAVI 7. 3GP 8. REAL VIDEO 9. MKV 10. FLV 11. F4V 12. RMVB 13. WebM 14. HDDVD 15. Blu-ray 16. qsv 99. 其他 （可多选）"]
[null,null,"图像传感器连续录制时间","ImageContinueRecordTime","h","Num","M","A2"]
[null,null,"图像传感器抗震动","ImageAntiVibration",null,"Str","R","B1",null,"eg:10至55Hz双向振幅1.5mmXYZ各方向2个小时"]
[null,null,"图像传感器抗冲击","ImageAntiImpact",null,"Str","R","B1",null,"eg:500m/s26个方向各3次"]
[null,null,"图像传感器控制模式","ImageCtrlType",null,"MEnum","R","D2","1. 外部触发 2. 程序切换 3. 错误区域 4. 外部标准图像注册 5. 辅助光源开关 99. 其他 （可多选）"]
[null,"运行参数","图像传感器是否输出视频","isImageRecord",null,"Boolv","S","L","0. 否 1. 是"]
[null,null,"图像传感器输出视频地址","ImageAddress",null,"Strv","S","L"]

{"sheet":"SEPF人流量传感器","index":12,"n_rows":59,"n_cols":10,"rows_kept":59,"cut":false,"hidden":false,"merged":[[48,0,58,0],[48,1,53,1],[54,1,58,1],[1,0,1,1],[0,0,0,9],[46,0,47,1],[2,0,45,1]]}
["人流量传感器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数-通用",null,"电源类型","PowerType",null,"MEnum","M","D2","1. 外接直流 2. 外接交流 3. 充电电池 4. 干电池 99. 其他 （可多选）"]
[null,null,"外接直流电压","ExDCU","V","Num","R","A2",null,"1.2V，1.5V，2V，3V，3.7V，11.1V，14.2V"]
[null,null,"外接交流电压/充电电压","ExACU","V","Num","R","A2"]
[null,null,"干电池型号","DryCellType","V","Enum","R","D1","1. AAAA 2. AAA 3. AA 4. A 5. SC 6. C 7. D 8. N 9. F 99. 其他"]
[null,null,"充电电池容量","RechargeBatteryCap","mAh","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"信号输出形式","SignType",null,"Enum","S","D1","1. 模拟信号 1.1 电压模拟信号 1.2 电流模拟信号 1.3 频率模拟信号 2. 数字信号\n2.1 电流数字信号 2.2 电压数字信号 2.3 频率数字信号 99. 其他"]
[null,null,"模拟信号输出电流范围","ASOutIRange","A","Num","R","A6"]
[null,null,"模拟信号输出电压范围","ASOutURange","V","Num","R","A6"]
[null,null,"模拟信号输出频率范围","ASOutFreqRange","Hz","Num","R","A6"]
[null,null,"数字信号输出高低电流","DSOutHLI","A","Num","R","A4"]
[null,null,"数字信号输出高低电平","DSOutHLU","V","Num","R","A4"]
[null,null,"数字信号输出高低频率","DSOutHLFreq","Hz","Num","R","A4"]
[null,null,"波特率","BaudRate",null,"Num","R","A1",null,"单片机或计算机在串口通信时的速率。指的是信号被调制以后在单位时间内的变化，即单位时间内载波参数变化的次数"]
[null,null,"是否有远传功能","isRemoteFunc",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否有无线传输功能","isWirelessFunc",null,"Bool ","S","E1","0. 否 1. 是"]
[null,null,"有线传输协议","WireTransProtocol",null,"Enum","M","D1","1. RS-232 2. RS-485 3. CAN总线 4. TCP/IP 5. ADSL 6. FSK 7. 光纤 8. 电力载波 99. 其他"]
[null,null,"无线传输协议","WirelessTransProtocol",null,"MEnum","M","D2","1. Zigbee 2. RFID 3. 蓝牙技术 4. NFC 5. WiFi 99. 其他 （可以多选）"]
[null,null,"有线传输距离","WireTransDistance","m","Num","R","A2"]
[null,null,"无线传输距离","WirelessTransDistance","m","Num","R","A2"]
[null,null,"有线传输功率","WireTransP","W","Num","R","A2"]
[null,null,"无线传输功率","WirelessTransP","W","Num","R","A2"]
[null,null,"是否有显示屏幕","isScreen",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有存储功能","isStorageFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"存储接口","StoragePort",null,"Enum","R","D1","1. USB 2. HDMI 3. SD卡 99. 其他"]
[null,null,"内存大小","MemorySize","GB","Num","R","A2"]
[null,null,"有无自动采样功能","IsAutosampleFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"自动采样时间间隔","AutosampleInterval","s","Num","R","A2"]
[null,null,"精密性","Precision","%FS","Num","M","A2"]
[null,null,"准确性","Accuracy","%FS","Num","R","A2"]
[null,null,"线性度","Linearity","%","Num","R","A2"]
[null,null,"零点偏置","ZeroOffset","mV","Num","R","A2"]
[null,null,"零点漂移","ZeroDrift","mV","Num","R","A2"]
[null,null,"长期稳定性","LongTermStability","%FS/年","Num","R","A2"]
[null,null,"响应时间","ResponseTime","s","Num","R","A2",null,"从测量下限升至测量上限63.2%所用时间"]
[null,null,"使用寿命","ServiceLife","年","Num","R","A2"]
[null,null,"电器保护类型","ElecProtectType",null,"MEnum","R","D2","1. 反向保护 2. 短路保护 3. 过载保护 99. 其他 （可多选）"]
[null,null,"安装方式","InstallType",null,"Enum","R","D1","1. 固定安装 1.1 焊接 1.2 螺纹连接 1.3 插接 2. 移动手持 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"标准工作压力","WorkPress","MPa","Num","R","A2"]
[null,null,"极限压力","ExtremePress","MPa","Num","R","A2"]
["运行参数-通用",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
["人流量传感器","技术参数","原理类型",null,null,"Enum","R","D1","1. 红外光电式 2. 多摄像头立体视觉式 3. 单摄像头式 4. RFID式 5. 移动设备式 99. 其他"]
[null,null,"用途类型",null,null,"MEnum","S","D2","1. 计量人流量 2. 监测室内人数 3. 人员位置监控 4. 入侵探测 99. 其他 （可多选）"]
[null,null,"是否有方向性",null,null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"是否特定人群",null,null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否能同时计量多人",null,null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"记录方式",null,null,"Enum","R","D1","1. 逐时记录 2. 记录改变量 3. 累计计数 99. 其他"]
[null,"运行参数","是否有人通过/靠近",null,null,"Enumv","S","L"," -1. 负向通过 0. 无 1. 正向通过/有人靠近"]
[null,null,"正向累计流量",null,"人次","Inst","M","L"]
[null,null,"负向累计流量",null,"人次","Inst","M","L"]
[null,null,"室内人数",null,"人","Inst","R","L"]
[null,null,"人员位置",null,null,"Attachmentv","R","L"]