{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["支路-调研-计算单元(电)","支路-调研-分项(水)","分项-计算单元-设备","支路-计算单元-FM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"支路-调研-计算单元(电)","index":0,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["调研使用信息ID","支路本地编码","进线号","备用进线号","关联仪表","仪表公式","变比","参与总支计算","计算单元本地编码","倒闸支路本地编码","支路设计容量/功率"]

{"sheet":"支路-调研-分项(水)","index":1,"n_rows":1,"n_cols":10,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["调研使用信息ID","支路本地编码","进线号","备用进线号","关联仪表","仪表公式","变比","参与总支计算","能耗模型ID","分项逻辑编码"]

{"sheet":"分项-计算单元-设备","index":2,"n_rows":1,"n_cols":4,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["计算单元本地编码","能耗模型ID","分项逻辑编码","设备本地编码"]

{"sheet":"支路-计算单元-FM","index":3,"n_rows":1,"n_cols":9,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["调研使用信息ID","本地编码(计算单元/支路)","类型(计算单元/支路)","ID(仪表号或计算单元本地编码)","支路或计算单元名称","FM设备本地编码","FM设备本地名称","FM设备安装位置","FM设备id"]