{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["VS视频监控系统","NP巡更系统","EG门禁系统","IA入侵报警系统"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"VS视频监控系统","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[[22,0,22,1],[23,0,23,1],[9,1,10,1],[14,0,21,0],[14,1,20,1],[0,0,0,9],[1,0,1,1],[2,0,13,0],[2,1,8,1],[11,1,13,1]]}
["视频监控系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","前端","摄像头类型","CameraType",null,"MEnum","S","D2","1. 普通模拟摄像头 2. 普通数字摄像头 3. 网络摄像头 99. 其他 （可多选）"]
[null,null,"摄像头转动辅助装置类型","CameraRotateType",null,"MEnum","M","D2","1. 云台 2. 智能球 99. 其他 （可多选）"]
[null,null,"信号类型","SignalType",null,"Enum","S","D1","1. 模拟信号 2. 数字信号 99. 其他"]
[null,null,"有无图像识别功能","isImageIdentifyFunc",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"有无防护罩","isShield",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"监控点数量","MonitoryPointNum","个","Num","M","A2"]
[null,null,"监控点位置","MonitoryPointLocation",null,"Attachment","R","F1"]
[null,"传输","视频传输方式","TransferType",null,"Enum","R","D1","1. 传输线缆传输 2. 同轴电缆 3. 光纤 4. 网线 99. 其他"]
[null,null,"传输协议","TransferProtocol",null,"Str","R","B1"]
[null,"显示","显示器数量","DisplayNum","台","Num","M","A2"]
[null,null,"视频存储容量","VideoStoreCap","TB","Num","M","A2"]
[null,null,"视频储存时间","MaxVideoStoreTime","天","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"报警状态","AlamStatus",null,"Enumvs","S","L","1. 正常 2. 报警 3. 试验 99. 其他"]
[null,null,"系统耗电功率","SysElecConsumP","kW","Inst","R","M"]
[null,null,"视频存档时间段","VideoStoreTime",null,"DTimer","M","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
["设定参数"]
["报警消息"]
[]
[]
[null,null,"  "]

{"sheet":"NP巡更系统","index":1,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[[12,0,12,1],[2,0,5,1],[0,0,0,9],[1,0,1,1],[6,0,10,1],[11,0,11,1]]}
["巡更系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"巡更系统分类","PatrolSysType",null,"Enum","S","D1","1. 接触式电子巡更 2. 感应式电子巡更 3. 在线式电子巡更 4. GPS巡检系统 99. 其他"]
[null,null,"巡更点数量","PatrolPointNum",null,"Num","M","A1"]
[null,null,"巡更点位置","PatrolPointLocation",null,"Attachment","R","F1"]
[null,null,"巡更路线","PatrolPath",null,"Attachment","R","F1"]
["运行状态",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"巡更点状态","PatrolPointStatus",null,"Enumvs","M","L","1. 未完成 2. 已完成无异常 3. 已完成上报异常 99. 其他"]
[null,null,"系统耗电功率","SysElecConsumP","kW","Inst","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"EG门禁系统","index":2,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[22,0,22,1],[23,0,23,1],[0,0,0,9],[1,0,1,1],[11,0,21,0],[11,1,19,1],[2,0,10,1],[20,1,21,1]]}
["门禁系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"组合方式","CombineMethod",null,"Enum","M","D1","1. 一体型 2. 分体型 99. 其他"]
[null,null,"门禁系统规模","SysScale",null,"Enum","M","D1","1. 小型门禁系统 2. 大型门禁系统 3. 局域网小型门禁系统 4. 局域网小型门禁系统 99. 其他"]
[null,null,"防护能力","DefendLev",null,"Enum","S","D1","1. A级 2. B级 3. C级 99. 其他"]
[null,null,"识读方式","RecognizeType",null,"MEnum","S","D2","1. 生物特征识别（指纹、眼底纹、虹膜、步态） 2. 数字密码识别 3. 磁卡识别 99. 其他 （可多选）"]
[null,null,"开门方式","OpenType",null,"Enum","M","D1","1. 单门双向 2. 双门双向 3. 四门单向 99. 其他"]
[null,null,"门锁方式","LockType",null,"Enum","R","D1","1. 电磁式 2. 门锁式 3. 门磁 99. 其他"]
[null,null,"电磁锁具供电方式","LockPowerType",null,"Enum","R","D1","1. 直流12V 2. 直流18V 3. 直流24V 99. 其他"]
[null,null,"门禁点数量","AccessCtrlNum","个","Num","M","A2"]
[null,null,"门禁位置","AccessCtrlLocation",null,"Attachment","R","F1"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"门禁点开关状态","SwitchStatus",null,"Boolvs","S","L","0. 关 1. 开"]
[null,null,"门禁点报警状态","AlarmStatus",null,"Enumvs","S","L","1. 正常 2. 报警 3. 试验 99. 其他"]
[null,null,"进入人流量","EnterFlow","人次/min","Inst","M","L"]
[null,null,"离开人流量","ExitFlow","人次/min","Inst","M","L"]
[null,null,"系统耗电功率","SysElecConsumP","kW","Inst","R","M"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计通过人次","AccPassPersonTime","人次","Acc","M","M"]
["设定参数"]
["报警消息"]

{"sheet":"IA入侵报警系统","index":3,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[[18,0,18,1],[0,0,0,9],[1,0,1,1],[2,0,9,1],[10,0,16,1],[17,0,17,1]]}
["入侵报警系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"报警器类型","AlertType",null,"MEnum","S","D2","1. 开关式警报器 2. 玻璃破碎式报警器 3. 空间移动式警报器（红外线、微波） 4. 手动报警装置 99. 其他 (可多选)"]
[null,null,"组建模式","BuildType",null,"Enum","R","D1","1. 分线式 2. 总线式 3. 无线制 4. 公共网络式 99. 其他"]
[null,null,"报警方式","AlarmType",null,"MEnum","S","D2","1. 声报警器 2. 光报警器 3. 震动报警器 99. 其他 （可多选）"]
[null,null,"防区数量","ZoneNum","个","Num","S","A2"]
[null,null,"防区划分","ZoneDivide",null,"Attachment","R","F1"]
[null,null,"探测器数量","DetectorNum","个","Num","M","A2"]
[null,null,"探测器位置","DetectorLocation",null,"Attachment","R","F1"]
[null,null,"布防时间","DeployTime","h","Num","R","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"报警状态","AlarmStatus",null,"Enumvs","S","L","1. 正常 2. 报警 3. 试验 99. 其他"]
[null,null,"系统耗电功率","SysElecConsumP","kW","Inst","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","R","M"]
["设定参数"]
["报警消息"]