{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["STLU污废水一体式提升机组","STSP潜污泵","STOR餐饮除油成套设备","STST化粪池","STCP集水坑"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"STLU污废水一体式提升机组","index":0,"n_rows":62,"n_cols":10,"rows_kept":62,"cut":false,"hidden":false,"merged":[[61,0,61,1],[58,0,60,1],[0,0,0,9],[1,0,1,1],[35,0,57,0],[24,1,34,1],[2,0,34,0],[35,1,52,1],[53,1,57,1],[2,1,23,1]]}
["污废水一体式提升机组"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","电源频率","PowerFreq","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定耗电功率","RatedP","kW","Num","S","A2"]
[null,null,"额定处理量","RatedTreatFlow","m3/h","Num","S","A2"]
[null,null,"最大处理量","MaxTreatFlow","m3/h","Num","S","A2"]
[null,null,"额定出口压力","RatedWaterOutPress","MPa","Num","M","A2"]
[null,null,"排污管直径","SewagePipeDiameter","mm","Num","R","A2"]
[null,null,"电机防护等级","MotorIPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"电机绝缘等级","MotorInsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"噪声强度","Noise","dB(A)","Num","M","A2"]
[null,null,"振动烈度","Vibration","mm/s","Num","M","A2"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
[null,null,"污水温度范围","SewageTempRange","℃","Numr","M","A6"]
[null,null,"污水PH值范围","SewagePHRange",null,"Numr","M","A5"]
[null,null,"污水密度范围","SewageRouRange","kg/m3","Numr","M","A6"]
[null,null,"污水固体颗粒最大直径","MaxParticleDiameter","mm","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
[null,"水泵","水泵类型","PumpType",null,"Enum","R","D1","1. 离心泵 2. 柱塞泵 3. 射流泵 4. 螺杆泵 99. 其他"]
[null,null,"是否有变频功能","isVFD",null,"Bool","S","E1","0. 定频 1. 变频"]
[null,null,"是否有档位选项","isGear",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"额定频率","PumpRatedFreq","Hz","Num","R","A2"]
[null,null,"额定扬程","PumpRatedHead","m","Num","S","A2"]
[null,null,"额定流量","PumpRatedFlow","m3/h","Num","S","A2"]
[null,null,"额定转速","PumpRatedRPM","rpm","Num","M","A2"]
[null,null,"水泵直径","PumpDiameter","mm","Num","R","A2",null,"口径"]
[null,null,"电机额定效率","PumpMotorRatedEff","%","Num","R","A2"]
[null,null,"水泵额定效率","PumpRatedEff","%","Num","R","A2"]
[null,null,"特性曲线","PumpCharacterCurve",null,"Attachment","R","F1"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","M","L"]
[null,null,"工作电流","I","A","Inst","M","L"]
[null,null,"运行频率","WorkFreq","Hz","Inst","M","L"]
[null,null,"工作档位","Gear",null,"Enumv","M","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","M","L"]
[null,null,"处理流量","SewageTreatFlow","m3/h","Inst","M","L"]
[null,null,"进口压力","SewageInPress","MPa","Inst","S","L"]
[null,null,"进口温度","SewageInTemp","℃","Inst","R","L"]
[null,null,"出口压力","SewageOutPress","MPa","Inst","S","L"]
[null,null,"出口温度","SewageOutTemp","℃","Inst","R","L"]
[null,null,"污水储量","SewageStoreVolume","m3","Inst","M","L"]
[null,null,"污水PH值","SewagePH",null,"Inst","R","L"]
[null,null,"污水密度","SewageRou","kg/m3","Inst","R","L"]
[null,"累计指标","累计提升水量","AccTreatVolume","m3","Acc","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数",null,"设备开关设定","EquipSwitchSet",null,"Boolp","S","L","0. 停止 1. 运行"]
[null,null,"设备频率设定","EquipFreqSet","Hz","Nump","S","L"]
[null,null,"设备档位设定","EquipGearSet",null,"Enump","S","L","1. 低档 2. 中档 3. 高档 99. 其他"]
["故障报警"]

{"sheet":"STSP潜污泵","index":1,"n_rows":66,"n_cols":10,"rows_kept":66,"cut":false,"hidden":false,"merged":[[65,0,65,1],[62,0,64,1],[35,1,38,1],[39,1,54,1],[0,0,0,9],[1,0,1,1],[39,0,61,0],[2,0,38,0],[55,1,56,1],[57,1,61,1],[2,1,34,1]]}
["潜污泵"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","电源频率","PowerFreq","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"额定频率","RatedFreq","Hz","Num","R","A2"]
[null,null,"水泵类型","PumpType",null,"Enum","R","D1","1. 离心泵 2. 柱塞泵 3. 射流泵 4. 螺杆泵 99. 其他"]
[null,null,"泵体安装类型","PumpInstallType",null,"Enum","R","D1","1. 立式 2. 卧式 99. 其他"]
[null,null,"处理污水类型","SewageTreatType",null,"Enum","M","D1","1. 切割式 2. 开式叶轮 3. 自动机搅拌式 4. WQ或QW型 99. 其他"]
[null,null,"调节类型","AdjustType",null,"Enum","M","D1","1. 定频无调节 2. 二档调节 3. 三档调节 4. 变频调节 99. 其他"]
[null,null,"是否为备用泵","isBackupPump",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否有变频功能","isVFD",null,"Bool","S","E1","0. 定频 1. 变频"]
[null,null,"是否有档位选项","isGear",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"额定扬程","RatedHead","m","Num","S","A2"]
[null,null,"额定流量","RatedFlow","m3/h","Num","S","A2"]
[null,null,"额定转速","RatedRPM","rpm","Num","M","A2"]
[null,null,"水泵直径","PumpDiameter","mm","Num","R","A2",null,"口径"]
[null,null,"电机额定效率","MotorRatedEff","%","Num","R","A2"]
[null,null,"水泵额定效率","PumpRatedEff","%","Num","R","A2"]
[null,null,"特性曲线","CharacterCurve",null,"Attachment","R","F1"]
[null,null,"电机防护等级","MotorIPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"电机绝缘等级","MotorInsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"噪声强度","Noise","dB(A)","Num","M","A2"]
[null,null,"振动烈度","Vibration","mm/s","Num","M","A2"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
[null,null,"污水温度范围","SewageTempRange","℃","Numr","M","A6"]
[null,null,"污水PH值范围","SewagePHRange",null,"Numr","M","A5"]
[null,null,"污水密度范围","SewageRouRange","kg/m3","Numr","M","A6"]
[null,null,"污水固体颗粒最大直径","MaxParticleDiameter","mm","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
[null,"辅助设备","变频器型号","VFDSpecification",null,"Str","R","B1"]
[null,null,"变频最高频率","VFDMaxFreq","Hz","Num","R","A2"]
[null,null,"变频最低频率","VFDMinFreq","Hz","Num","R","A2"]
[null,null,"搅拌直径","StirDiameter","m","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"运行电压","U","V","Inst","M","L"]
[null,null,"运行电流","I","A","Inst","M","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","M","L",null,"三相有功功率"]
[null,null,"运行频率","Freq","Hz","Inst","M","L"]
[null,null,"工作档位","Gear",null,"Enumv","M","L","1. 低档 2. 中档 3. 高档 99. 其他"]
[null,null,"瞬时流量","Flow","m3/h","Inst","R","L"]
[null,null,"水泵进口压力","SewageInPress","MPa","Inst","S","L"]
[null,null,"水泵出口压力","SewageOutPress","MPa","Inst","S","L"]
[null,null,"水泵扬程","Head","m","Inst","R","M"]
[null,null,"污水PH值","SewagePH",null,"Inst","R","L"]
[null,null,"污水密度","SewageRou","kg/m3","Inst","R","L"]
[null,"瞬时指标","电机效率","MotorEff","%","Inst","R","M"]
[null,null,"水泵效率","PumpEff","%","Inst","R","M"]
[null,"累计指标","累计输送介质量","AccTreatVolume","m3","Acc","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数",null,"设备开关设定","EquipSwitchSet",null,"Boolp","S","L","0. 停止 1. 运行"]
[null,null,"设备频率设定","EquipFreqSet","Hz","Nump","S","L"]
[null,null,"设备档位设定","EquipGearSet",null,"Enump","S","L","1. 低档 2. 中档 3. 高档 99. 其他"]
["故障报警"]

{"sheet":"STOR餐饮除油成套设备","index":2,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[63,1,64,1],[2,0,16,1],[0,0,0,9],[1,0,1,1],[17,0,35,0],[30,1,35,1],[17,1,28,1],[36,0,36,1],[37,0,37,1]]}
["餐饮除油成套设备"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"电源频率","PowerFreq","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"最大处理流量","MaxTreatFlow","m3/h","Num","S","A2"]
[null,null,"额定除油效率","RatedEff","%","Num","M","A2"]
[null,null,"可分离油的比重","OilSpecificGravity",null,"Num","R","A1"]
[null,null,"浮选级数","FlotationLev","级","Num","R","A2"]
[null,null,"气液比","GasLiquidRatio",null,"Num","R","A1",null,"与浮选级数一起决定除油效率"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
[null,null,"污水温度范围","SewageTempRange","℃","Numr","M","A6"]
[null,null,"污水PH值范围","SewagePHRange",null,"Numr","M","A5"]
[null,null,"污水密度范围","SewageRouRange","kg/m3","Numr","M","A6"]
[null,null,"污水固体颗粒最大直径","MaxParticleDiameter","mm","Num","M","A2"]
[null,null,"理论压力损失","RatedPressLost","Pa","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","M","L"]
[null,null,"工作电流","I","A","Inst","M","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","M","L"]
[null,null,"处理流量","TreatFlow","m3/h","Inst","R","L"]
[null,null,"进水含油浓度","SewageInOil","mg/L","Inst","R","L"]
[null,null,"出水含油浓度","SewageOutOil ","mg/L","Inst","R","L"]
[null,null,"截油量","RemoveOil","mg/L","Inst","R","L"]
[null,"瞬时指标","除油效率","RemoveOilEff","%","Inst","R","M"]
[null,"累计指标","累计处理水量","AccTreatVolume","m3","Acc","R","M"]
[null,null,"累计截油量","AccRemoveOil","kg","Acc","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"STST化粪池","index":3,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[[31,0,31,1],[32,0,32,1],[0,0,0,9],[1,0,1,1],[16,0,30,0],[16,1,28,1],[29,1,30,1],[2,0,15,1]]}
["化粪池"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"化粪池长度","BasinLength","m","Num","M","A2"]
[null,null,"化粪池宽度","BasinWidth","m","Num","M","A2"]
[null,null,"化粪池深度","BasinDepth","m","Num","M","A2"]
[null,null,"最大容积","BasinCap","m3","Num","S","A2"]
[null,null,"进水孔直径","InHoleDiameter","mm","Num","R","A2"]
[null,null,"进水孔深度","InHoleDepth","m","Num","R","A2"]
[null,null,"出水孔直径","OutHoleDiameter","mm","Num","R","A2"]
[null,null,"出水孔深度","OutHoleDepth","m","Num","R","A2"]
[null,null,"通气孔直径","VentHoleDiameter","mm","Num","R","A2"]
[null,null,"检查孔直径","InspectHoleDiameter","mm","Num","R","A2"]
[null,null,"杂质去除率","DeImpurityRatio","%","Num","R","A2"]
[null,null,"固体浓度范围","SolidConcentrateRange","mg/L","Numr","R","A6"]
[null,null,"有机物浓度范围","OrganismConcentrateRange","mg/L","Numr","R","A6"]
[null,null,"清掏周期","RatedCleanPeriod","天","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"进水流量","SewageInFlow","m3/h","Inst","R","L"]
[null,null,"出水流量","SewageOutFlow","m3/h","Inst","R","L"]
[null,null,"出气量","GasOutFlow","m3/h","Inst","R","L"]
[null,null,"池内水位",null,"m3","Inst","M"]
[null,null,"处理前固体浓度","BeforeTreatSolidConcentrate","mg/L","Inst","R","L"]
[null,null,"处理前有机物浓度","BeforeTreatOrganismConcentrate","mg/L","Inst","R","L"]
[null,null,"处理后固体浓度","AfterTreatSolidConcentrate","mg/L","Inst","R","L"]
[null,null,"处理后有机物浓度","AfterTreatOrganismConcentrate","mg/L","Inst","R","L"]
[null,"累计指标","污水停留时间","SewageHRT","h","Acc","R","M"]
[null,null,"距上次污泥清挖时间","CleanPeriod","天","Acc","M","M"]
["设定参数"]
["报警消息"]

{"sheet":"STCP集水坑","index":4,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[10,0,19,1],[0,0,0,9],[1,0,1,1],[2,0,9,1],[22,0,23,1],[20,0,21,1]]}
["集水坑"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"集水坑长度","SumpLength","m","Num","M","A2"]
[null,null,"集水坑宽度","SumpWidth","m","Num","M","A2"]
[null,null,"集水坑深度","SumpDepth","m","Num","M","A2"]
[null,null,"最大容积","SumpCap","m3","Num","S","A2"]
[null,null,"进水孔直径","InHoleDiameter","mm","Num","R","A2"]
[null,null,"进水孔深度","InHoleDepth","m","Num","R","A2"]
[null,null,"出水孔直径","OutHoleDiameter","mm","Num","R","A2"]
[null,null,"出水孔深度","OutHoleDepth","m","Num","R","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"进水流量","SewageInFlow","m3/h","Inst","M","L"]
[null,null,"出水流量","SewageOutFlow","m3/h","Inst","R","L"]
[null,null,"出气量","GasOutFlow","m3/h","Inst","R","L"]
[null,null,"池内水位","BasinLevel","m","Inst","S","L"]
[null,null,"池内水位档位","BasinLevelGear",null,"Enumv","S","L"]
["设定参数",null,"低液位报警高度设定","LowLevelSet","m","Nump","S"]
[null,null,"高液位报警高度设定","HighLevelSet","m","Nump","S"]
["报警消息",null,"低液位报警","LowLevelAlarm",null,"Boolp","S"]
[null,null,"高液位报警","HighLevelAlarm",null,"Boolp","S"]