{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["TDHSIP综合保护装置","TDLSDW低压配电抽屉"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDHSIP综合保护装置","index":0,"n_rows":319,"n_cols":10,"rows_kept":319,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[185,1,288,1],[2,0,7,1],[289,1,305,1],[306,1,317,1],[8,0,317,0],[10,1,27,1],[28,1,37,1],[39,1,54,1],[55,1,62,1],[63,1,184,1]]}
["综合保护装置"]
["分级标签",null,"信息点","信息点编码","单位","类型","输入方式","优先级","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","kV","Num","A2"]
[null,null,"额定电流","RatedI","A","Num","A2"]
[null,null,"额定功率","RatedP","kW","Num","A2"]
[null,null,"额定频率","RatedFreq","Hz","Num","A2"]
[null,null,"相保护电流","PhaseProtectI","A","Num","A2"]
[null,null,"保护单元","ProtectUnit",null,"Enum","D2",null,"1. 空气断路器 2. 零序电流互感器 3. 回路电流互感器 4. 直流稳压电源 5. 电磁脱扣装置 6. 二次侧的过压和欠压保护单元 7. 脱扣开关控制单元 8. 漏电保护单元 9. 时基单元 10. 音响报警单元 11. 过流保护单元 12. 倍载延时单元 13. 短路保护单元 14. 其他 （可多选）"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","L",null,"0. 停止 1. 运行"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","L",null,"1. 本地手动 2. 本地自动 3. 远程手动 4. 远程自动 5. 其他"]
[null,"电压","I母A相电压","1BusAPhaseU","kV","Inst","L",null,null,"或A相电压"]
[null,null,"I母B相电压","1BusBPhaseU","kV","Inst","L",null,null,"或B相电压"]
[null,null,"I母C相电压","1BusCPhaseU","kV","Inst","L",null,null,"或C相电压"]
[null,null,"I母Uab线电压","1BusUabU","kV","Inst","L",null,null,"或Uab线电压"]
[null,null,"I母Ubc线电压","1BusUbcU","kV","Inst","L",null,null,"或Ubc线电压"]
[null,null,"I母Uac线电压","1BusUacU","kV","Inst","L",null,null,"或Uac线电压"]
[null,null,"I母正序电压","1BusPositiveSequenceU","kV","Inst","L",null,null,"或正序电压"]
[null,null,"I母负序电压","1BusNegativeSequenceU","kV","Inst","L",null,null,"或负序电压"]
[null,null,"I母零序电压","1BusZeroSequenceU","kV","Inst","L",null,null,"或零序电压"]
[null,null,"II母A相电压","2BusAPhaseU","kV","Inst","L"]
[null,null,"II母B相电压","2BusBPhaseU","kV","Inst","L"]
[null,null,"II母C相电压","2BusCPhaseU","kV","Inst","L"]
[null,null,"II母Uab线电压","2BusUabU","kV","Inst","L"]
[null,null,"II母Ubc线电压","2BusUbcU","kV","Inst","L"]
[null,null,"II母Uac线电压","2BusUacU","kV","Inst","L"]
[null,null,"II母正序电压","2BusPositiveSequenceU","kV","Inst","L"]
[null,null,"II母负序电压","2BusNegativeSequenceU","kV","Inst","L"]
[null,null,"II母零序电压","2BusZeroSequenceU","kV","Inst","L"]
[null,"电流","A相电流","APhaseI","A","Inst","L"]
[null,null,"B相电流","BPhaseI","A","Inst","L"]
[null,null,"C相电流","CPhaseI","A","Inst","L"]
[null,null,"A相无功电流","APhaseReactiveI","A","Inst","L"]
[null,null,"B相无功电流","BPhaseReactiveI","A","Inst","L"]
[null,null,"C相无功电流","CPhaseReactiveI","A","Inst","L"]
[null,null,"中性线电流","NeutralI","A","Inst","L"]
[null,null,"正序电流","PositiveSequenceI","A","Inst","L"]
[null,null,"负序电流","NegativeSequenceI","A","Inst","L"]
[null,null,"零序电流","ZeroSequenceI","A","Inst","L"]
[null,null,"频率","Freq","Hz","Inst","L"]
[null,"功率","A相有功功率","APhaseActiveP","kW","Inst","L"]
[null,null,"B相有功功率","BPhaseActiveP","kW","Inst","L"]
[null,null,"C相有功功率","CPhaseActiveP","kW","Inst","L"]
[null,null,"总有功功率","TotActiveP","kW","Inst","L"]
[null,null,"A相无功功率","APhaseReactiveP","kVar","Inst","L"]
[null,null,"B相无功功率","BPhaseReactiveP","kVar","Inst","L"]
[null,null,"C相无功功率","CPhaseReactiveP","kVar","Inst","L"]
[null,null,"总无功功率","TotReactiveP","kVar","Inst","L"]
[null,null,"A相视在功率","APhaseApparentP","kVA","Inst","L"]
[null,null,"B相视在功率","BPhaseApparentP","kVA","Inst","L"]
[null,null,"C相视在功率","CPhaseApparentP","kVA","Inst","L"]
[null,null,"总视在功率","TotApparentP","kVA","Inst","L"]
[null,null,"A相功率因数","APhasePFactor",null,"Inst","L"]
[null,null,"B相功率因数","BPhasePFactor",null,"Inst","L"]
[null,null,"C相功率因数","CPhasePFactor",null,"Inst","L"]
[null,null,"总功率因数","TotPFactor",null,"Inst","L"]
[null,"总谐波","总谐波A相电压","TotHarmonicAPhaseU","kV","Inst","L"]
[null,null,"总谐波B相电压","TotHarmonicBPhaseU","kV","Inst","L"]
[null,null,"总谐波C相电压","TotHarmonicCPhaseU","kV","Inst","L"]
[null,null,"总电压谐波含量","TotUHarmonic","kV","Inst","L"]
[null,null,"总谐波A相电流","TotHarmonicAPhaseI","A","Inst","L"]
[null,null,"总谐波B相电流","TotHarmonicBPhaseI","A","Inst","L"]
[null,null,"总谐波C相电流","TotHarmonicCPhaseI","A","Inst","L"]
[null,null,"总电流谐波含量","TotIHarmonic","A","Inst","L"]
[null,"畸变率","A相电压谐波畸变率","APhaseUHD","%","Inst","L"]
[null,null,"B相电压谐波畸变率","BPhaseUHD","%","Inst","L"]
[null,null,"C相电压谐波畸变率","CPhaseUHD","%","Inst","L"]
[null,null,"电压谐波总畸变率","UTHD","%","Inst","L"]
[null,null,"A相电流谐波畸变率","APhaseIHD","%","Inst","L"]
[null,null,"B相电流谐波畸变率","BPhaseIHD","%","Inst","L"]
[null,null,"C相电流谐波畸变率","CPhaseIHD","%","Inst","L"]
[null,null,"电流谐波总畸变率","ITHD","%","Inst","L"]
[null,null,"3阶谐波A相电压畸变率","3APhaseUHD","%","Inst","L"]
[null,null,"3阶谐波B相电压畸变率","3BPhaseUHD","%","Inst","L"]
[null,null,"3阶谐波C相电压畸变率","3CPhaseUHD","%","Inst","L"]
[null,null,"3阶谐波A相电流畸变率","3APhaseIHD","%","Inst","L"]
[null,null,"3阶谐波B相电流畸变率","3BPhaseIHD","%","Inst","L"]
[null,null,"3阶谐波C相电流畸变率","3CPhaseIHD","%","Inst","L"]
[null,null,"5阶谐波A相电压畸变率","5APhaseUHD","%","Inst","L"]
[null,null,"5阶谐波B相电压畸变率","5BPhaseUHD","%","Inst","L"]
[null,null,"5阶谐波C相电压畸变率","5CPhaseUHD","%","Inst","L"]
[null,null,"5阶谐波A相电流畸变率","5APhaseIHD","%","Inst","L"]
[null,null,"5阶谐波B相电流畸变率","5BPhaseIHD","%","Inst","L"]
[null,null,"5阶谐波C相电流畸变率","5CPhaseIHD","%","Inst","L"]
[null,null,"7阶谐波A相电压畸变率","7APhaseUHD","%","Inst","L"]
[null,null,"7阶谐波B相电压畸变率","7BPhaseUHD","%","Inst","L"]
[null,null,"7阶谐波C相电压畸变率","7CPhaseUHD","%","Inst","L"]
[null,null,"7阶谐波A相电流畸变率","7APhaseIHD","%","Inst","L"]
[null,null,"7阶谐波B相电流畸变率","7BPhaseIHD","%","Inst","L"]
[null,null,"7阶谐波C相电流畸变率","7CPhaseIHD","%","Inst","L"]
[null,null,"9阶谐波A相电压畸变率","9APhaseUHD","%","Inst","L"]
[null,null,"9阶谐波B相电压畸变率","9BPhaseUHD","%","Inst","L"]
[null,null,"9阶谐波C相电压畸变率","9CPhaseUHD","%","Inst","L"]
[null,null,"9阶谐波A相电流畸变率","9APhaseIHD","%","Inst","L"]
[null,null,"9阶谐波B相电流畸变率","9BPhaseIHD","%","Inst","L"]
[null,null,"9阶谐波C相电流畸变率","9CPhaseIHD","%","Inst","L"]
[null,null,"11阶谐波A相电压畸变率","11APhaseUHD","%","Inst","L"]
[null,null,"11阶谐波B相电压畸变率","11BPhaseUHD","%","Inst","L"]
[null,null,"11阶谐波C相电压畸变率","11CPhaseUHD","%","Inst","L"]
[null,null,"11阶谐波A相电流畸变率","11APhaseIHD","%","Inst","L"]
[null,null,"11阶谐波B相电流畸变率","11BPhaseIHD","%","Inst","L"]
[null,null,"11阶谐波C相电流畸变率","11CPhaseIHD","%","Inst","L"]
[null,null,"13阶谐波A相电压畸变率","13APhaseUHD","%","Inst","L"]
[null,null,"13阶谐波B相电压畸变率","13BPhaseUHD","%","Inst","L"]
[null,null,"13阶谐波C相电压畸变率","13CPhaseUHD","%","Inst","L"]
[null,null,"13阶谐波A相电流畸变率","13APhaseIHD","%","Inst","L"]
[null,null,"13阶谐波B相电流畸变率","13BPhaseIHD","%","Inst","L"]
[null,null,"13阶谐波C相电流畸变率","13CPhaseIHD","%","Inst","L"]
[null,null,"15阶谐波A相电压畸变率","15APhaseUHD","%","Inst","L"]
[null,null,"15阶谐波B相电压畸变率","15BPhaseUHD","%","Inst","L"]
[null,null,"15阶谐波C相电压畸变率","15CPhaseUHD","%","Inst","L"]
[null,null,"15阶谐波A相电流畸变率","15APhaseIHD","%","Inst","L"]
[null,null,"15阶谐波B相电流畸变率","15BPhaseIHD","%","Inst","L"]
[null,null,"15阶谐波C相电流畸变率","15CPhaseIHD","%","Inst","L"]
[null,null,"17阶谐波A相电压畸变率","17APhaseUHD","%","Inst","L"]
[null,null,"17阶谐波B相电压畸变率","17BPhaseUHD","%","Inst","L"]
[null,null,"17阶谐波C相电压畸变率","17CPhaseUHD","%","Inst","L"]
[null,null,"17阶谐波A相电流畸变率","17APhaseIHD","%","Inst","L"]
[null,null,"17阶谐波B相电流畸变率","17BPhaseIHD","%","Inst","L"]
[null,null,"17阶谐波C相电流畸变率","17CPhaseIHD","%","Inst","L"]
[null,null,"19阶谐波A相电压畸变率","19APhaseUHD","%","Inst","L"]
[null,null,"19阶谐波B相电压畸变率","19BPhaseUHD","%","Inst","L"]
[null,null,"19阶谐波C相电压畸变率","19CPhaseUHD","%","Inst","L"]
[null,null,"19阶谐波A相电流畸变率","19APhaseIHD","%","Inst","L"]
[null,null,"19阶谐波B相电流畸变率","19BPhaseIHD","%","Inst","L"]
[null,null,"19阶谐波C相电流畸变率","19CPhaseIHD","%","Inst","L"]
[null,null,"21阶谐波A相电压畸变率","21APhaseUHD","%","Inst","L"]
[null,null,"21阶谐波B相电压畸变率","21BPhaseUHD","%","Inst","L"]
[null,null,"21阶谐波C相电压畸变率","21CPhaseUHD","%","Inst","L"]
[null,null,"21阶谐波A相电流畸变率","21APhaseIHD","%","Inst","L"]
[null,null,"21阶谐波B相电流畸变率","21BPhaseIHD","%","Inst","L"]
[null,null,"21阶谐波C相电流畸变率","21CPhaseIHD","%","Inst","L"]
[null,null,"23阶谐波A相电压畸变率","23APhaseUHD","%","Inst","L"]
[null,null,"23阶谐波B相电压畸变率","23BPhaseUHD","%","Inst","L"]
[null,null,"23阶谐波C相电压畸变率","23CPhaseUHD","%","Inst","L"]
[null,null,"23阶谐波A相电流畸变率","23APhaseIHD","%","Inst","L"]
[null,null,"23阶谐波B相电流畸变率","23BPhaseIHD","%","Inst","L"]
[null,null,"23阶谐波C相电流畸变率","23CPhaseIHD","%","Inst","L"]
[null,null,"25阶谐波A相电压畸变率","25APhaseUHD","%","Inst","L"]
[null,null,"25阶谐波B相电压畸变率","25BPhaseUHD","%","Inst","L"]
[null,null,"25阶谐波C相电压畸变率","25CPhaseUHD","%","Inst","L"]
[null,null,"25阶谐波A相电流畸变率","25APhaseIHD","%","Inst","L"]
[null,null,"25阶谐波B相电流畸变率","25BPhaseIHD","%","Inst","L"]
[null,null,"25阶谐波C相电流畸变率","25CPhaseIHD","%","Inst","L"]
[null,null,"27阶谐波A相电压畸变率","27APhaseUHD","%","Inst","L"]
[null,null,"27阶谐波B相电压畸变率","27BPhaseUHD","%","Inst","L"]
[null,null,"27阶谐波C相电压畸变率","27CPhaseUHD","%","Inst","L"]
[null,null,"27阶谐波A相电流畸变率","27APhaseIHD","%","Inst","L"]
[null,null,"27阶谐波B相电流畸变率","27BPhaseIHD","%","Inst","L"]
[null,null,"27阶谐波C相电流畸变率","27CPhaseIHD","%","Inst","L"]
[null,null,"29阶谐波A相电压畸变率","29APhaseUHD","%","Inst","L"]
[null,null,"29阶谐波B相电压畸变率","29BPhaseUHD","%","Inst","L"]
[null,null,"29阶谐波C相电压畸变率","29CPhaseUHD","%","Inst","L"]
[null,null,"29阶谐波A相电流畸变率","29APhaseIHD","%","Inst","L"]
[null,null,"29阶谐波B相电流畸变率","29BPhaseIHD","%","Inst","L"]
[null,null,"29阶谐波C相电流畸变率","29CPhaseIHD","%","Inst","L"]
[null,null,"31阶谐波A相电压畸变率","31APhaseUHD","%","Inst","L"]
[null,null,"31阶谐波B相电压畸变率","31BPhaseUHD","%","Inst","L"]
[null,null,"31阶谐波C相电压畸变率","31CPhaseUHD","%","Inst","L"]
[null,null,"31阶谐波A相电流畸变率","31APhaseIHD","%","Inst","L"]
[null,null,"31阶谐波B相电流畸变率","31BPhaseIHD","%","Inst","L"]
[null,null,"31阶谐波C相电流畸变率","31CPhaseIHD","%","Inst","L"]
[null,null,"33阶谐波A相电压畸变率","33APhaseUHD","%","Inst","L"]
[null,null,"33阶谐波B相电压畸变率","33BPhaseUHD","%","Inst","L"]
[null,null,"33阶谐波C相电压畸变率","33CPhaseUHD","%","Inst","L"]
[null,null,"33阶谐波A相电流畸变率","33APhaseIHD","%","Inst","L"]
[null,null,"33阶谐波B相电流畸变率","33BPhaseIHD","%","Inst","L"]
[null,null,"33阶谐波C相电流畸变率","33CPhaseIHD","%","Inst","L"]
[null,null,"35阶谐波A相电压畸变率","35APhaseUHD","%","Inst","L"]
[null,null,"35阶谐波B相电压畸变率","35BPhaseUHD","%","Inst","L"]
[null,null,"35阶谐波C相电压畸变率","35CPhaseUHD","%","Inst","L"]
[null,null,"35阶谐波A相电流畸变率","35APhaseIHD","%","Inst","L"]
[null,null,"35阶谐波B相电流畸变率","35BPhaseIHD","%","Inst","L"]
[null,null,"35阶谐波C相电流畸变率","35CPhaseIHD","%","Inst","L"]
[null,null,"37阶谐波A相电压畸变率","37APhaseUHD","%","Inst","L"]
[null,null,"37阶谐波B相电压畸变率","37BPhaseUHD","%","Inst","L"]
[null,null,"37阶谐波C相电压畸变率","37CPhaseUHD","%","Inst","L"]
[null,null,"37阶谐波A相电流畸变率","37APhaseIHD","%","Inst","L"]
[null,null,"37阶谐波B相电流畸变率","37BPhaseIHD","%","Inst","L"]
[null,null,"37阶谐波C相电流畸变率","37CPhaseIHD","%","Inst","L"]
[null,null,"39阶谐波A相电压畸变率","39APhaseUHD","%","Inst","L"]
[null,null,"39阶谐波B相电压畸变率","39BPhaseUHD","%","Inst","L"]
[null,null,"39阶谐波C相电压畸变率","39CPhaseUHD","%","Inst","L"]
[null,null,"39阶谐波A相电流畸变率","39APhaseIHD","%","Inst","L"]
[null,null,"39阶谐波B相电流畸变率","39BPhaseIHD","%","Inst","L"]
[null,null,"39阶谐波C相电流畸变率","39CPhaseIHD","%","Inst","L"]
[null,"保护","断路器分/合闸状态","BreakerStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"I母断路器分/合闸状态","1BusBreakerStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"II母断路器分/合闸状态","2BusBreakerStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"分段开关分/合闸状态","SectionSwitchStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"负荷开关状态","LoadSwitchStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"接触器状态","ContactorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"隔离开关状态","DisconnectorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"I母上隔离开关状态","Bus1UpDisconnectorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"I母下隔离开关状态","Bus1DownDisconnectorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"II母上隔离开关状态","Bus2UpDisconnectorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"II母下隔离开关状态","Bus2DownDisconnectorStatus",null,"Boolv","L",null,"0. 分闸 1. 合闸"]
[null,null,"接地状态","GroundStatus",null,"Boolv","L",null,"0. 正常接地 1. 接地故障"]
[null,null,"检修状态","OverhaulStatus",null,"Boolv","L",null,"0. 正常工作 1. 检修"]
[null,null,"弹簧储能状态","SpringEStoreStatus",null,"Boolv","L",null,"0. 正常储能 1. 未储能"]
[null,null,"绝缘状态","InsulationStatus",null,"Boolv","L",null,"0. 正常绝缘 1. 绝缘故障"]
[null,null,"I段绝缘状态","Section1InsulationStatus",null,"Boolv","L",null,"0. 正常绝缘 1. 绝缘故障"]
[null,null,"II段绝缘状态","Section2InsulationStatus",null,"Boolv","L",null,"0. 正常绝缘 1. 绝缘故障"]
[null,null,"重合闸充电状态","ReclosingChargeStatus",null,"Boolv","L",null,"0. 已充满电 1. 正在充电"]
[null,null,"通讯状态","CommunicateStatus",null,"Boolv","L",null,"0. 正常通讯 1. 通讯故障"]
[null,null,"工作位上隔离","WorkLocationUpIsolation",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"试验位下隔离","TestLocationDownIsolation",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"控制电源开入状态","CtrlPowerSwitchStatus",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"I母线TV合位","Bus1TVSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"II母线TV合位","Bus2TVSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"进线1跳位开入","In1TripSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"进线2跳位开入","In2TripSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"手动并列","ManualParallelSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"手动解列","ManualSplitSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"低压解列","LUSplitSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"TV自动并列","TVAutoParallelSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"闭锁投分段","BlockSectionSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"闭锁投进线1","BlockIn1Switch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"闭锁投进线2","BlockIn2Switch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"手车1开关状态","Handcart1Switch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"手车2开关状态","Handcart2Switch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"备自投方式动作","SpareAutoSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"备自投方式动作不成功","SpareAutoFailSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"压力释放","PressReliefSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"I进线过负荷投入","In1OverloadSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"II进线过负荷投入","In2OverloadSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"三相一次重合闸","3Phase1ShotReclosureSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"闭锁重合闸","BlockReclosureSwitch",null,"Boolv","L",null,"0. 正常 1. 动作"]
[null,null,"前加速保护","ForwardAccelerateProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"后加速保护","BackwardAccelerateProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"绝缘监测保护","InsulationMonitorProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"过流保护","OverIProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"过流加速保护","OverIAccelerateProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过流保护","ZeroSequenceOverIProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过压保护","ZeroSequenceOverUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"电动机起动超时保护","MotorStartOverTimeProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"过热保护","OverTempProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"过电压保护","OverUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"低电压保护","LowUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"不平衡电压保护","UnbalanceUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"不平衡电流保护","UnbalanceIProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"过负荷保护","OverLoadProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"短路保护","ShortCircuitProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"低周减载保护","LowFreqLoadReductionProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"负序过流I段保护","NegativeSequenceOverISection1Protect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"反时限过流保护","InverseTimeOverIProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"非电量保护","NonElecProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"速断保护","InstTripProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"限时速断保护","TimeLimitInstTripProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过流I段保护","ZeroSequenceOverISection1Protect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过流II段保护","ZeroSequenceOverISection2Protect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过流III段保护","ZeroSequenceOverISection3Protect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"零序过流III段反时限保护","ZeroSequenceOverISection3InverseTimeProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"PT失压保护","PTULossProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"I母PT失压保护","Bus1PTULossProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"II母PT失压保护","Bus2PTULossProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"负控跳闸保护","LoadCtrlTripProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"重瓦斯保护","HeavyGasProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"轻瓦斯保护","LightGasProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"堵转保护","RotorLockProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"I母过电压保护","Bus1OverUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"II母过电压保护","Bus2OverUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"I母低电压保护","Bus1LowUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"II母低电压保护","Bus2LowUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"I母接地电压保护","Bus1GroundUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"II母接地电压保护","Bus2GroundUProtect",null,"Boolv","L",null,"0. 正常 1. 保护"]
[null,null,"控制回路异常告警","CtrlCircuitAbnormityAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"控制回路断线告警","CtrlCircuitBreakAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"母线TV断线告警","BusTVBreakAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"TA断线告警","TABreakAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"装置故障告警","DeviceFaultAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"接地报警","GroundAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"跳位异常告警","TripAbnormityAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"过流告警","OverIAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"过流加速告警","OverIAccelerateAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"零序过流告警","ZeroSequenceOverIAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"零序过压告警","ZeroSequenceOverUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"过热告警","OverTempAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"过电压告警","OverUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"低电压告警","LowUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"不平衡电压告警","UnbalanceUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"不平衡电流告警","UnbalanceIAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"过负荷告警","OverLoadAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"主变开门告警","MainTransOpenDoorAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"I母PT断线告警","Bus1PTBreakAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"II母PT断线告警","Bus2PTBreakAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"I母过电压告警","Bus1OverUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"II母过电压告警","Bus2OverUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"I母低电压告警","Bus1LowUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,null,"II母低电压告警","Bus2LowUAlarm",null,"Boolv","L",null,"0. 正常 1. 报警"]
[null,"关键指标","负载负荷率","LoadRate","%","Inst","M"]
[null,null,"配电容量负荷率","CapRate","%","Inst","M"]
[null,null,"三相不平衡电压","3PhaseUnbalancedU","kV","Inst","M"]
[null,null,"三线不平衡电压","3LineUnbalancedU","kV","Inst","M"]
[null,null,"三相不平衡电流","3PhaseUnbalancedI","A","Inst","M"]
[null,null,"最大不平衡线电压","MaxUnbalanceLineU","kV","Inst","M"]
[null,null,"最大不平衡相电压","MaxUnbalancePhaseU","kV","Inst","M"]
[null,null,"最大不平衡电流","MaxUnbalanceI","A","Inst","M"]
[null,null,"电压不平衡度","UUnbalanceRate","%","Inst","M"]
[null,null,"电流不平衡度","IUnbalanceRate","%","Inst","M"]
[null,null,"A相电压偏差","APhaseUDeviation","%","Inst","M"]
[null,null,"B相电压偏差","BPhaseUDeviation","%","Inst","M"]
[null,null,"C相电压偏差","CPhaseUDeviation","%","Inst","M"]
[null,null,"ab线电压偏差","LineabUDeviation","%","Inst","M"]
[null,null,"bc线电压偏差","LinebcUDeviation","%","Inst","M"]
[null,null,"ca线电压偏差","LinecaUDeviation","%","Inst","M"]
[null,null,"频率偏差","FreqDeviation","Hz","Inst","M"]
[null,"累计参数","正向有功电能","AccPositiveActiveE","kWh","Acc","M"]
[null,null,"反向有功电能","AccReverseActiveE","kWh","Acc","M"]
[null,null,"正向无功电能","AccPositiveReactiveE","kVarh","Acc","M"]
[null,null,"反向无功电能","AccReverseReactiveE","kVarh","Acc","M"]
[null,null,"视在电能","AccApparentE","kVAh","Acc","M"]
[null,null,"净累计有功电能","NetAccActiveE","kWh","Acc","M"]
[null,null,"净累计无功电能","NetAccReactiveE","kVarh","Acc","M"]
[null,null,"感性无功电能","AccInductiveReactiveE","kVarh","Acc","M"]
[null,null,"容性无功电能","AccCapacitiveReactiveE","kVarh","Acc","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","M"]
["设定参数",null,null,"SetPara",null,"Step","Y"]

{"sheet":"TDLSDW低压配电抽屉","index":1,"n_rows":228,"n_cols":9,"rows_kept":228,"cut":false,"hidden":false,"merged":[[20,1,30,1],[15,1,17,1],[0,0,0,8],[1,0,1,1],[2,1,7,1],[18,0,226,0],[31,1,39,1],[40,1,50,1],[52,1,67,1],[68,1,75,1],[198,1,214,1],[2,0,17,0],[215,1,226,1],[8,1,11,1],[12,1,14,1],[76,1,197,1]]}
["低压配电抽屉"]
["分级标签",null,"信息点","信息点编码","单位","类型","输入方式","字典选择"," 备注"]
["技术参数","总体","低压配电抽屉类型","LowUCabDrawerType",null,"Enum","D1","1. GCK 2. GCS 3. MNS 4. 其他","GGD是固定柜，GCK、GCS、MNS是抽屉柜；GCK和GCS、MNS抽屉推进机构不同；GCS只能单面操作，MNS可以双面操作"]
[null,null,"额定电压","RatedU","V","Num","A2"]
[null,null,"额定电流","RatedI","A","Num","A2"]
[null,null,"额定功率","RatedP","kW","Num","A2"]
[null,null,"额定频率","RatedFreq","Hz","Num","A2"]
[null,null,"相保护电流","PhaseProtectI","A","Num","A2"]
[null,"开关保护","是否包含负荷开关","isLoadSwitch",null,"Bool","E1","0. 无 1. 有"]
[null,null,"是否包含熔断器","isFuse",null,"Bool","E1","0. 无 1. 有"]
[null,null,"是否包含断路器","isBreaker",null,"Bool","E1","0. 无 1. 有"]
[null,null,"是否包含漏电保护器","isLeakageProtector",null,"Bool","E1","0. 无 1. 有"]
[null,"电压互感器","是否包含电压互感器","isUTrans",null,"Bool","E1","0. 无 1. 有"]
[null,null,"电压互感器额定电压比","UTransRatedURatio",null,"Num","A1"]
[null,null,"电压互感器准确级组合","UTransAccuracyCombination",null,"Enum","D1","1. 0.2级 2. 0.5级 3. 1级 4. 3级 5. 3P级 6. 6P级 7. 其他","0.2，0.5，1，3为测量用；3P，6P为保护用"]
[null,"电流互感器","是否包含电流互感器","isITrans",null,"Bool","E1","0. 无 1. 有"]
[null,null,"电流互感器类型","ITransType",null,"Enum","D1","1. 单匝式 2. 穿墙式 3. 支柱式 4. 母线式 5. 复匝式 6. 其他"]
[null,null,"电流互感器额定电流比","ITransRatedIRatio",null,"Num","A1"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","L","0.停止 1.运行"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","L","1.本地手动 2.本地自动 3.远程手动 4.远程自动 5. 其他"]
[null,"开关状态","断路器分/合闸状态","BreakerStatus",null,"Boolv","L","0. 分闸 1. 合闸"]
[null,null,"分段开关分/合闸状态","SectionSwitchStatus",null,"Boolv","L","0. 分闸 1. 合闸"]
[null,null,"负荷开关状态","LoadSwitchStatus",null,"Boolv","L","0. 分闸 1. 合闸"]
[null,null,"接触器状态","ContactorStatus",null,"Boolv","L","0. 分闸 1. 合闸"]
[null,null,"隔离开关状态","DisconnectorStatus",null,"Boolv","L","0. 分闸 1. 合闸"]
[null,null,"接地状态","GroundStatus",null,"Boolv","L","0. 正常接地 1. 接地故障"]
[null,null,"检修状态","OverhaulStatus",null,"Boolv","L","0. 正常工作 1. 检修"]
[null,null,"弹簧储能状态","SpringEStoreStatus",null,"Boolv","L","0. 正常储能 1. 未储能"]
[null,null,"绝缘状态","InsulationStatus",null,"Boolv","L","0. 正常绝缘 1. 绝缘故障"]
[null,null,"重合闸充电状态","ReclosingChargeStatus",null,"Boolv","L","0. 已充满电 1. 正在充电"]
[null,null,"通讯状态","CommunicateStatus",null,"Boolv","L","0. 正常通讯 1. 通讯故障"]
[null,"电压","A相电压","APhaseU","V","Inst","L"]
[null,null,"B相电压","BPhaseU","V","Inst","L"]
[null,null,"C相电压","CPhaseU","V","Inst","L"]
[null,null,"Uab线电压","UabU","V","Inst","L"]
[null,null,"Ubc线电压","UbcU","V","Inst","L"]
[null,null,"Uac线电压","UacU","V","Inst","L"]
[null,null,"正序电压","PositiveSequenceU","V","Inst","L"]
[null,null,"负序电压","NegativeSequenceU","V","Inst","L"]
[null,null,"零序电压","ZeroSequenceU","V","Inst","L"]
[null,"电流","A相测量电流","APhaseI","A","Inst","L"]
[null,null,"B相测量电流","BPhaseI","A","Inst","L"]
[null,null,"C相测量电流","CPhaseI","A","Inst","L"]
[null,null,"A相无功电流","APhaseReactiveI","A","Inst","L"]
[null,null,"B相无功电流","BPhaseReactiveI","A","Inst","L"]
[null,null,"C相无功电流","CPhaseReactiveI","A","Inst","L"]
[null,null,"中性线电流","NeutralI","A","Inst","L"]
[null,null,"正序电流","PositiveSequenceI","A","Inst","L"]
[null,null,"负序电流","NegativeSequenceI","A","Inst","L"]
[null,null,"高压零序电流","HUZeroSequenceI","A","Inst","L"]
[null,null,"低压零序电流","LUZeroSequenceI","A","Inst","L"]
[null,null,"频率","Freq","Hz","Inst","L"]
[null,"功率","A相有功功率","APhaseActiveP","kW","Inst","L"]
[null,null,"B相有功功率","BPhaseActiveP","kW","Inst","L"]
[null,null,"C相有功功率","CPhaseActiveP","kW","Inst","L"]
[null,null,"总有功功率","TotActiveP","kW","Inst","L"]
[null,null,"A相无功功率","APhaseReactiveP","kVar","Inst","L"]
[null,null,"B相无功功率","BPhaseReactiveP","kVar","Inst","L"]
[null,null,"C相无功功率","CPhaseReactiveP","kVar","Inst","L"]
[null,null,"总无功功率","TotReactiveP","kVar","Inst","L"]
[null,null,"A相视在功率","APhaseApparentP","kVA","Inst","L"]
[null,null,"B相视在功率","BPhaseApparentP","kVA","Inst","L"]
[null,null,"C相视在功率","CPhaseApparentP","kVA","Inst","L"]
[null,null,"总视在功率","TotApparentP","kVA","Inst","L"]
[null,null,"A相功率因数","APhasePFactor",null,"Inst","L"]
[null,null,"B相功率因数","BPhasePFactor",null,"Inst","L"]
[null,null,"C相功率因数","CPhasePFactor",null,"Inst","L"]
[null,null,"总功率因数","TotPFactor",null,"Inst","L"]
[null,"总谐波","总谐波A相电压","TotHarmonicAPhaseU","V","Inst","L"]
[null,null,"总谐波B相电压","TotHarmonicBPhaseU","V","Inst","L"]
[null,null,"总谐波C相电压","TotHarmonicCPhaseU","V","Inst","L"]
[null,null,"总电压谐波含量","TotUHarmonic","V","Inst","L"]
[null,null,"总谐波A相电流","TotHarmonicAPhaseI","A","Inst","L"]
[null,null,"总谐波B相电流","TotHarmonicBPhaseI","A","Inst","L"]
[null,null,"总谐波C相电流","TotHarmonicCPhaseI","A","Inst","L"]
[null,null,"总电流谐波含量","TotIHarmonic","A","Inst","L"]
[null,"畸变率","A相电压谐波畸变率","APhaseUHD","%","Inst","L"]
[null,null,"B相电压谐波畸变率","BPhaseUHD","%","Inst","L"]
[null,null,"C相电压谐波畸变率","CPhaseUHD","%","Inst","L"]
[null,null,"电压谐波总畸变率","UTHD","%","Inst","L"]
[null,null,"A相电流谐波畸变率","APhaseIHD","%","Inst","L"]
[null,null,"B相电流谐波畸变率","BPhaseIHD","%","Inst","L"]
[null,null,"C相电流谐波畸变率","CPhaseIHD","%","Inst","L"]
[null,null,"电流谐波总畸变率","ITHD","%","Inst","L"]
[null,null,"3阶谐波A相电压畸变率","3APhaseUHD","%","Inst","L"]
[null,null,"3阶谐波B相电压畸变率","3BPhaseUHD","%","Inst","L"]
[null,null,"3阶谐波C相电压畸变率","3CPhaseUHD","%","Inst","L"]
[null,null,"3阶谐波A相电流畸变率","3APhaseIHD","%","Inst","L"]
[null,null,"3阶谐波B相电流畸变率","3BPhaseIHD","%","Inst","L"]
[null,null,"3阶谐波C相电流畸变率","3CPhaseIHD","%","Inst","L"]
[null,null,"5阶谐波A相电压畸变率","5APhaseUHD","%","Inst","L"]
[null,null,"5阶谐波B相电压畸变率","5BPhaseUHD","%","Inst","L"]
[null,null,"5阶谐波C相电压畸变率","5CPhaseUHD","%","Inst","L"]
[null,null,"5阶谐波A相电流畸变率","5APhaseIHD","%","Inst","L"]
[null,null,"5阶谐波B相电流畸变率","5BPhaseIHD","%","Inst","L"]
[null,null,"5阶谐波C相电流畸变率","5CPhaseIHD","%","Inst","L"]
[null,null,"7阶谐波A相电压畸变率","7APhaseUHD","%","Inst","L"]
[null,null,"7阶谐波B相电压畸变率","7BPhaseUHD","%","Inst","L"]
[null,null,"7阶谐波C相电压畸变率","7CPhaseUHD","%","Inst","L"]
[null,null,"7阶谐波A相电流畸变率","7APhaseIHD","%","Inst","L"]
[null,null,"7阶谐波B相电流畸变率","7BPhaseIHD","%","Inst","L"]
[null,null,"7阶谐波C相电流畸变率","7CPhaseIHD","%","Inst","L"]
[null,null,"9阶谐波A相电压畸变率","9APhaseUHD","%","Inst","L"]
[null,null,"9阶谐波B相电压畸变率","9BPhaseUHD","%","Inst","L"]
[null,null,"9阶谐波C相电压畸变率","9CPhaseUHD","%","Inst","L"]
[null,null,"9阶谐波A相电流畸变率","9APhaseIHD","%","Inst","L"]
[null,null,"9阶谐波B相电流畸变率","9BPhaseIHD","%","Inst","L"]
[null,null,"9阶谐波C相电流畸变率","9CPhaseIHD","%","Inst","L"]
[null,null,"11阶谐波A相电压畸变率","11APhaseUHD","%","Inst","L"]
[null,null,"11阶谐波B相电压畸变率","11BPhaseUHD","%","Inst","L"]
[null,null,"11阶谐波C相电压畸变率","11CPhaseUHD","%","Inst","L"]
[null,null,"11阶谐波A相电流畸变率","11APhaseIHD","%","Inst","L"]
[null,null,"11阶谐波B相电流畸变率","11BPhaseIHD","%","Inst","L"]
[null,null,"11阶谐波C相电流畸变率","11CPhaseIHD","%","Inst","L"]
[null,null,"13阶谐波A相电压畸变率","13APhaseUHD","%","Inst","L"]
[null,null,"13阶谐波B相电压畸变率","13BPhaseUHD","%","Inst","L"]
[null,null,"13阶谐波C相电压畸变率","13CPhaseUHD","%","Inst","L"]
[null,null,"13阶谐波A相电流畸变率","13APhaseIHD","%","Inst","L"]
[null,null,"13阶谐波B相电流畸变率","13BPhaseIHD","%","Inst","L"]
[null,null,"13阶谐波C相电流畸变率","13CPhaseIHD","%","Inst","L"]
[null,null,"15阶谐波A相电压畸变率","15APhaseUHD","%","Inst","L"]
[null,null,"15阶谐波B相电压畸变率","15BPhaseUHD","%","Inst","L"]
[null,null,"15阶谐波C相电压畸变率","15CPhaseUHD","%","Inst","L"]
[null,null,"15阶谐波A相电流畸变率","15APhaseIHD","%","Inst","L"]
[null,null,"15阶谐波B相电流畸变率","15BPhaseIHD","%","Inst","L"]
[null,null,"15阶谐波C相电流畸变率","15CPhaseIHD","%","Inst","L"]
[null,null,"17阶谐波A相电压畸变率","17APhaseUHD","%","Inst","L"]
[null,null,"17阶谐波B相电压畸变率","17BPhaseUHD","%","Inst","L"]
[null,null,"17阶谐波C相电压畸变率","17CPhaseUHD","%","Inst","L"]
[null,null,"17阶谐波A相电流畸变率","17APhaseIHD","%","Inst","L"]
[null,null,"17阶谐波B相电流畸变率","17BPhaseIHD","%","Inst","L"]
[null,null,"17阶谐波C相电流畸变率","17CPhaseIHD","%","Inst","L"]
[null,null,"19阶谐波A相电压畸变率","19APhaseUHD","%","Inst","L"]
[null,null,"19阶谐波B相电压畸变率","19BPhaseUHD","%","Inst","L"]
[null,null,"19阶谐波C相电压畸变率","19CPhaseUHD","%","Inst","L"]
[null,null,"19阶谐波A相电流畸变率","19APhaseIHD","%","Inst","L"]
[null,null,"19阶谐波B相电流畸变率","19BPhaseIHD","%","Inst","L"]
[null,null,"19阶谐波C相电流畸变率","19CPhaseIHD","%","Inst","L"]
[null,null,"21阶谐波A相电压畸变率","21APhaseUHD","%","Inst","L"]
[null,null,"21阶谐波B相电压畸变率","21BPhaseUHD","%","Inst","L"]
[null,null,"21阶谐波C相电压畸变率","21CPhaseUHD","%","Inst","L"]
[null,null,"21阶谐波A相电流畸变率","21APhaseIHD","%","Inst","L"]
[null,null,"21阶谐波B相电流畸变率","21BPhaseIHD","%","Inst","L"]
[null,null,"21阶谐波C相电流畸变率","21CPhaseIHD","%","Inst","L"]
[null,null,"23阶谐波A相电压畸变率","23APhaseUHD","%","Inst","L"]
[null,null,"23阶谐波B相电压畸变率","23BPhaseUHD","%","Inst","L"]
[null,null,"23阶谐波C相电压畸变率","23CPhaseUHD","%","Inst","L"]
[null,null,"23阶谐波A相电流畸变率","23APhaseIHD","%","Inst","L"]
[null,null,"23阶谐波B相电流畸变率","23BPhaseIHD","%","Inst","L"]
[null,null,"23阶谐波C相电流畸变率","23CPhaseIHD","%","Inst","L"]
[null,null,"25阶谐波A相电压畸变率","25APhaseUHD","%","Inst","L"]
[null,null,"25阶谐波B相电压畸变率","25BPhaseUHD","%","Inst","L"]
[null,null,"25阶谐波C相电压畸变率","25CPhaseUHD","%","Inst","L"]
[null,null,"25阶谐波A相电流畸变率","25APhaseIHD","%","Inst","L"]
[null,null,"25阶谐波B相电流畸变率","25BPhaseIHD","%","Inst","L"]
[null,null,"25阶谐波C相电流畸变率","25CPhaseIHD","%","Inst","L"]
[null,null,"27阶谐波A相电压畸变率","27APhaseUHD","%","Inst","L"]
[null,null,"27阶谐波B相电压畸变率","27BPhaseUHD","%","Inst","L"]
[null,null,"27阶谐波C相电压畸变率","27CPhaseUHD","%","Inst","L"]
[null,null,"27阶谐波A相电流畸变率","27APhaseIHD","%","Inst","L"]
[null,null,"27阶谐波B相电流畸变率","27BPhaseIHD","%","Inst","L"]
[null,null,"27阶谐波C相电流畸变率","27CPhaseIHD","%","Inst","L"]
[null,null,"29阶谐波A相电压畸变率","29APhaseUHD","%","Inst","L"]
[null,null,"29阶谐波B相电压畸变率","29BPhaseUHD","%","Inst","L"]
[null,null,"29阶谐波C相电压畸变率","29CPhaseUHD","%","Inst","L"]
[null,null,"29阶谐波A相电流畸变率","29APhaseIHD","%","Inst","L"]
[null,null,"29阶谐波B相电流畸变率","29BPhaseIHD","%","Inst","L"]
[null,null,"29阶谐波C相电流畸变率","29CPhaseIHD","%","Inst","L"]
[null,null,"31阶谐波A相电压畸变率","31APhaseUHD","%","Inst","L"]
[null,null,"31阶谐波B相电压畸变率","31BPhaseUHD","%","Inst","L"]
[null,null,"31阶谐波C相电压畸变率","31CPhaseUHD","%","Inst","L"]
[null,null,"31阶谐波A相电流畸变率","31APhaseIHD","%","Inst","L"]
[null,null,"31阶谐波B相电流畸变率","31BPhaseIHD","%","Inst","L"]
[null,null,"31阶谐波C相电流畸变率","31CPhaseIHD","%","Inst","L"]
[null,null,"33阶谐波A相电压畸变率","33APhaseUHD","%","Inst","L"]
[null,null,"33阶谐波B相电压畸变率","33BPhaseUHD","%","Inst","L"]
[null,null,"33阶谐波C相电压畸变率","33CPhaseUHD","%","Inst","L"]
[null,null,"33阶谐波A相电流畸变率","33APhaseIHD","%","Inst","L"]
[null,null,"33阶谐波B相电流畸变率","33BPhaseIHD","%","Inst","L"]
[null,null,"33阶谐波C相电流畸变率","33CPhaseIHD","%","Inst","L"]
[null,null,"35阶谐波A相电压畸变率","35APhaseUHD","%","Inst","L"]
[null,null,"35阶谐波B相电压畸变率","35BPhaseUHD","%","Inst","L"]
[null,null,"35阶谐波C相电压畸变率","35CPhaseUHD","%","Inst","L"]
[null,null,"35阶谐波A相电流畸变率","35APhaseIHD","%","Inst","L"]
[null,null,"35阶谐波B相电流畸变率","35BPhaseIHD","%","Inst","L"]
[null,null,"35阶谐波C相电流畸变率","35CPhaseIHD","%","Inst","L"]
[null,null,"37阶谐波A相电压畸变率","37APhaseUHD","%","Inst","L"]
[null,null,"37阶谐波B相电压畸变率","37BPhaseUHD","%","Inst","L"]
[null,null,"37阶谐波C相电压畸变率","37CPhaseUHD","%","Inst","L"]
[null,null,"37阶谐波A相电流畸变率","37APhaseIHD","%","Inst","L"]
[null,null,"37阶谐波B相电流畸变率","37BPhaseIHD","%","Inst","L"]
[null,null,"37阶谐波C相电流畸变率","37CPhaseIHD","%","Inst","L"]
[null,null,"39阶谐波A相电压畸变率","39APhaseUHD","%","Inst","L"]
[null,null,"39阶谐波B相电压畸变率","39BPhaseUHD","%","Inst","L"]
[null,null,"39阶谐波C相电压畸变率","39CPhaseUHD","%","Inst","L"]
[null,null,"39阶谐波A相电流畸变率","39APhaseIHD","%","Inst","L"]
[null,null,"39阶谐波B相电流畸变率","39BPhaseIHD","%","Inst","L"]
[null,null,"39阶谐波C相电流畸变率","39CPhaseIHD","%","Inst","L"]
[null,"关键指标","负载负荷率","LoadRate","%","Inst","M"]
[null,null,"配电容量负荷率","CapRate","%","Inst","M"]
[null,null,"三相不平衡电压","3PhaseUnbalancedU","V","Inst","M"]
[null,null,"三线不平衡电压","3LineUnbalancedU","V","Inst","M"]
[null,null,"三相不平衡电流","3PhaseUnbalancedI","A","Inst","M"]
[null,null,"最大不平衡线电压","MaxUnbalanceLineU","V","Inst","M"]
[null,null,"最大不平衡相电压","MaxUnbalancePhaseU","V","Inst","M"]
[null,null,"最大不平衡电流","MaxUnbalanceI","A","Inst","M"]
[null,null,"电压不平衡度","UUnbalanceRate","%","Inst","M"]
[null,null,"电流不平衡度","IUnbalanceRate","%","Inst","M"]
[null,null,"A相电压偏差","APhaseUDeviation","%","Inst","M"]
[null,null,"B相电压偏差","BPhaseUDeviation","%","Inst","M"]
[null,null,"C相电压偏差","CPhaseUDeviation","%","Inst","M"]
[null,null,"ab线电压偏差","LineabUDeviation","%","Inst","M"]
[null,null,"bc线电压偏差","LinebcUDeviation","%","Inst","M"]
[null,null,"ca线电压偏差","LinecaUDeviation","%","Inst","M"]
[null,null,"频率偏差","FreqDeviation","Hz","Inst","M"]
[null,"累计参数","正向有功电能","AccPositiveActiveE","kWh","Acc","M"]
[null,null,"反向有功电能","AccReverseActiveE","kWh","Acc","M"]
[null,null,"正向无功电能","AccPositiveReactiveE","kVarh","Acc","M"]
[null,null,"反向无功电能","AccReverseReactiveE","kVarh","Acc","M"]
[null,null,"视在电能","AccApparentE","kVAh","Acc","M"]
[null,null,"净累计有功电能","NetAccActiveE","kWh","Acc","M"]
[null,null,"净累计无功电能","NetAccReactiveE","kVarh","Acc","M"]
[null,null,"感性无功电能","AccInductiveReactiveE","kVarh","Acc","M"]
[null,null,"容性无功电能","AccCapacitiveReactiveE","kVarh","Acc","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","M"]
["设定参数",null,null,"SetPara",null,"Step","Y"]